  CONFIGURATION EDITOR
  IP REDIRECTION WITHOUT RIP

# IP Routing

ARP Settings

Enable IP Routing

IP-DTE Address Mapping

IP Frame Priority

IP QOS

Poison Reverse

RIP Metric Policy

RIP Options

RIP V2 Authentication

RIP V2 Summary

Static Routes

Subnet Masks

Transmit / Receive RIP

Routing Summary

Transmit/Receive RIP Packets

Enable IP Routing

  Enable (select) this feature if you intend to route IP frames through the unit. If this feature is enabled, IP bridging must be disabled.
  Range: Enabled or Disabled

Transmit/Receive RIP Packets

  This parameter enables you to control whether the unit can transmit Routing Information Protocol (RIP) packets or act on any received RIP packets. To change the current setting, click the down arrow to display a list of options, then click your selection.
  Range: Transmit, Receive, Neither, or Both

Enable IP Routing

  Enable (select) this feature if you intend to route IP frames through the unit. If this feature is enabled, IP bridging must be disabled.
  Range: Enabled or Disabled

IP Frame Priority

  This parameter sets the priority of IP frames routed over frame relay ports.
  Range: Low, Medium, High, or Urgent

ARP Settings

  These options enable you to select which ARP format the specified port should generate, and whether or not the unit should act as a Proxy ARP agent on that port.

Poison Reverse

  This option enables you to activate poison reverse on a frame relay port.

Routing Summary

  This option enables you to indicate whether or not summary information is
  generated in the RIP on the specified port.

Static Routes

  This feature enables you to enter static routes for routers that do not use RIP, or routes that do not change.

Subnet Masks

  This feature enables you to define a series of addresses that use a particular subnet address. This ensures there is no confusion as to which network a packet must be forwarded.

Transmit / Receive RIP

  This feature enables you to override the Transmit/Receive RIP setting for specific interfaces.

RIP Options

  These parameters enable you to configure RIP Settings on a port-level basis.

RIP V2 Authentication

  These parameters enable to you define the values for RIP V2 Authentication.

RIP V2 Summary

  These parameters enable you to define what is sent in the RIP V2 Summary packet.

IP QOS

  These parameters enable you to define the values used for Quality of Service.

RIP Metric Policy

  These parameters enable you to set values for RIP metrics.

IP-DTE Address Mapping

  This feature is used for routing IP frames over an X25 network. It enables you to assign an IP address to a DTE interface.