#

# EDITOR HOME

# NETWORK PORT

# FRAP Network Port

#### BPV Thresholding

#### Circuit Identifier

#### Clock Source

#### Network Loop Rate

#### Network Mode

  Defines the type of service provided on the attached network line.
  Range: Dedicated, Frame Relay

#### Network Loop Rate

  Defines the network loop speed for the attached network line.
  Range: 56-Kbps, or 64-Kbps

#### Circuit Identifier

  Defines the network circuit identifier of the carrier service provider.
  Range: 0 ~ 30 alpha-numeric characters

#### Clock Source

  Identifies the source of the network timing clock. The clock source may be obtained from the network line, or an internal clock crystal.
  Notes: In a point-to-point application, make certain one unit is configured for network timing and the other for internal timing. In a point-to-network application, make certain the unit is configured for network timing.
  Range: Internal or Network

#### BPV Thresholding

  Defines the Bi-Polar Violation (BPV) function that, when set to 10E-4, generates an alarm or SNMP Trap after detecting violations exceeding the pre-defined threshold.
  Range: At 10e-4 or Disabled