  CONFIGURATION EDITOR
  IPX ROUTING

# Static SAPs For IPX Routing

DLCI

Network Number

Node Address

Number of Hops

Port

Server Name

Server Network Number

Service Type

Socket Address

  This is an advanced feature set used to fine tune the network. To configure a static SAP, you must know several things about the Novell service identified by the SAP.
  To add and entry, click on the Add button.
  To delete an entry, select the entry you want to delete, then click on the Delete button.

Port

  This field defines the port on which you want to create a static SAP.
  Range: 1 -- 8 or LAN

DLCI

  The DLCI number must match the one assigned to the frame relay port. If you are connecting two FRADs back-to-back, use DLCI number 32 on both ends.
  Range: 16 -- 1023

Network Number

  This is the number assigned to the specified port and/or DLCI. All frame relay ports use network number 00000000 (unnumbered RIP).
  Range: 8 hexadecimal numbers

Service Type

  This is the type of service provided on the specified virtual port. For example, file servers are type 0004.
  Range: 4 hexadecimal numbers

Server Name

  This field defines the name of the Novell server connected to the specified virtual port.
  Range: Up to 48 characters

Server Network Number

  This field defines the network number assigned to the specified local Novell server.
  Range: 8 hexadecimal numbers

Node Address

  This field defines the MAC address of the remote Novell server.
  Range: 12 hexadecimal numbers

Socket Address

  This is the IPX socket address assigned to the specified service.
  Range: 4 hexadecimal numbers

Number of Hops

  This is the number of times a datagram passes through a router when transmitting from its source to its destination.
  Range: 0-F hexadecimal