# CONFIGURATION EDITOR

# IP ROUTING

# RIP V2 Authentication

Method

  This value defines the type of password to use.
  Range: Password, MD5, or None.

Key or Password

  This field defines the key or password that authenticates the packet.
  Range: 1~16 alphanumeric characters.

Start Time

  This field identifies the start date and time for the specified authorization key. If the method type is not set to MD5, this field is ignored.
  Range: In the format of MMDDYYYYHHMMSS

End Time

  This field identifies that ending date and time for the specified authorization key. If the method type is not set to MD5, this field is ignored.
  Range: In the format of MMDDYYYYHHMMSS