# CONFIGURATION EDITOR

# IP ROUTING

# IP Routing To DTE

Port

  Click inside this field to select the port that is attached to the DTE device for which you are assigning the IP address.
  Range: Any WAN port

DTE Address

  This field defines the DTE address for which you want to assign an IP Address.
  Range: 0 ~ 1023

IP Address

  This field defines the IP address you want to assign to the specified DTE Address.
  Range: Four numbers (0 ~ 255) separated by three periods