  CONFIGURATION EDITOR
  IP ROUTING

# ARP Settings For IP Routing

ARP Settings

  This parameter defines the ARP format that should be generated on the specified port
  .
  Range: None, Auto, Inverse, Routed, Token Ring Bridged, Ethernet II Bridged, or 802.3 Bridged.
  If Auto is selected, the unit sends an Inverse ARP and Routed ARP for routed environments, and all three bridged ARP formats for bridged environments.
  In a normal routed environment, only Routed ARP should be sent.
  Inverse ARP is always sent when a DLCI is activated in both routed and bridged environments.

Act as Proxy ARP Agent

  This parameter is applicable for frame relay and dial backup ports. It defines whether or not Proxy ARP is enabled for frame relay-attached devices.
  This feature enables a head-end FRAD to act as a proxy agent for a branch office FRAD.
  Range: Enabled or Disabled