  CONFIGURATION EDITOR
  BRIDGING

# BPDU Transmission

Transmit BPDUs

  Enable (select) this feature if you want BPDUs to transmit over all DLCIs.
  You may also enable this option if you intend to transmit BPDUs over several DLCIs. To disable BPDU transmission over the DLCIs that do not participate in the spanning tree, you must add them to the Virtual-Port Overrides list.
  This option does not have to be enabled to add DLCIs to the Virtual-Port Overrides list.
  Range: Enabled or Disabled

Virtual-Port Overrides

  This list enables you to specify which DLCIs the BPDU must transmit over.
  1. Click on the Add button.
  2. Click inside the Port field if you want to select another port from the pop-up list.
  3. Click inside the DLCI field and enter the provider-assigned DLCI number.
  4. Click inside the Transmit BPDUs field, to set the filtering to Yes or No.
  Range: Ports: 1 -- 8, or LAN, DLCI's: 16 -- 1023, Transmit BPDUs: Yes or No