  CONFIGURATION EDITOR
  FILTERING

# ARP Filter

  To add an entry, click on the Add button.

Port

  This field enables you to select a valid Frame Relay port.

DLCI Low

  This field defines the lowest DLCI number to include for this entry.
  Range: 16 ~ 1023

DLCI High

  This field defines the highest DLCI number to include for this entry.
  Range: 16 ~ 1023

Forward / Discard

  This field enables you to select whether to forward or discard ARP frames for the specified port and DLCI parameters.
  Range: Forward or Discard