  CONFIGURATION EDITOR

# VNIP Parameters

Port Number

VNIP Hello

VNIP Support

  Note: The R7 FrameNode requires only two configuration parameters per port and only a single port is supported at this time.

Port Number

  This combo box will present a drop list of the configured Frame Relay Ports. When a port is selected, the other controls are updated to reflect the current settings for the selected port.
  Range: 1~4 (Currently only one port supported)

VNIP Support

  This combo box corresponds to the VNIP circuit management parameter (VNP)
  Range: Disabled or Enabled.
  Note: When the parameter is configured to DISABLED, the circuit management function is completely turned off for this port. It is recommended to the user that VNP be DISABLED on the Head End FrameNode frame relay ports. Access Configuration Editor validation will check that VNIP is enabled for at most 1 Frame Relay port.

VNIP Hello

  This combo box corresponds to the VNIP Hello (VNH) parameter. This parameter instructs the FrameNode to initiate or not initiate "hello" messages on the frame relay link.
  Range: Active or Passive