#

# EDITOR HOME

# MAINTENANCE PORT

# FRAP 3.0 Maintenance Port

#### Communication Mode

#### Data Bits

#### Data Rate

#### Flow Control

#### Parity

#### Stop Bits

####

#### Communication Mode

  VT100 supports a VT-100-compatible ASCII terminal for local unit programming/control.
  SLIP supports an attachment to a DTE device for remote SNMP, or Telnet programming/control.
  CSLIP supports an attachment to a CSLIP-type device for remote SNMP, or Telnet programming/control.
  Range: ASCII-VT100, SLIP, or CSLIP

#### Data Rate

  This field defines the rate at which the port communicates with the attached device.
  Range: 2400, 9600, or 19200-Bps

#### Parity

  This field defines the type of parity used to check transfers. None indicates that character words are sent without parity.
  Range: None, Odd, or Even

#### Data Bits

  This field defines the number of data bits used by each character word.
  Range: 8 or 7 bits

#### Stop Bits

  This field defines the number of stop bits used by each character word.
  Range: 1, 1.5, or 2 bits

#### Flow Control

  Flow Control can be adjusted to one of the following parameters:
  Range: None, Software, or Hardware