# Unit Detail

# Unit Monitoring

# Displaying Short Term Statistics

#### Done

#### Stop/Start

#### Update

#### Displaying Short Term Statistics

  The FRAP AND T-FRAP monitor and collect Short Term statistics on Frame Relay traffic passing across each DLCI. Packet traffic is monitored and statistical counts taken for Layer 2 throughput, Layer 3 application protocol-based, socket-level IP protocols, and other protocols defined by supported filters. Short Term statistics reflect the running totals (receive and transmit counts) of all DLCIs. To display a breakdown of the current interval counts on individual DLCIs.
  To display Short Term statistics (in tabular form):
  1 Position the mouse arrow over the Unit Detail window's graphical representation of the COMM port, and click the right mouse button.
  2 Select Short Term Statistics - All DLCIs from the list of pull-down menu options.
  3 Select, from the list of pull-down options, the category of Short Term DLCI statistics you wish to view, and click the left mouse button.
  This action will cause a window, corresponding to your selection, to be displayed.
  Note: The window values displayed in parentheses represents the difference (delta) between values obtained during the previous polling interval and the current interval.
  The buttons located at the bottom of each Short Term DLCI statistics window are described in the following paragraphs.
  Stop/Start - Clicking this button stops and starts the statistics polling action.
  Update - Clicking this button will update (refresh) the information contained in the Short Term DLCI statistics window.
  Done - Clicking this button will close the Short Term DLCI statistics window.