  CONFIGURATION EDITOR
  SERIAL PORT
  ACCESS PORT

# Bisync RJE Port

Advanced

Carrier

Clocking

Connect Type

Destination

DLCI

Map to Port

NAU Name

Initial State

Retry Count (N2)

Reply Timeout

Signal Control

Speed

XID

  Note: Depending upon your product type, this dialog may vary. This help context covers all possible configuration parameters. If your dialog does not contain certain parameters, they don't apply to the product you are configuring.

NAU Name

  This optional field enables you to assign a name to the port. NAU names must be unique to the unit.
  Range: Up to eight alphanumeric characters

Initial State

  This option defines the port's state at system startup. If disabled, an operator must manually enable the port.
  Range: Disabled

Carrier

  This selects the type of carrier used by the port.
  Range: Switched (modem), or Constant

Clocking

  This option determines whether the port uses internal or external clocking.
  Range: Internal, External, X.21 Internal, or X.21 External

Speed

  This value determines the speed at which the port operates. If the port is externally clocked, the speed is determined by the clocking device, providing it doesn't exceed the maximum rate.
  Range: Dependent upon the attached devices

Signal Control

  Click on this button to define the conditions which determine the port's status.

Reply Timeout

  This parameter defines the length of time the port waits for a response from the attached RJE station.
  Range: 1 -- 10 seconds

Retry Count (N2)

  This value defines the number of times the unit attempts to complete a protocol exchange with a connected device before failing it. This prevents the unit from prematurely failing devices due to a temporary loss of response.
  Range: 1 -- 20 times

XID

  This field enables you to define an XID address, used to establish LLC sessions.
  Range: 8 hexadecimal numbers

Destination

  Click on this button to select the destination device. If the device does not appear in the list, you may add it through the Destination Editor.
  Range: Any destination from the list.

Map to Port

  This is the port number through which the destination is contacted.
  Range: 1 -- 8

DLCI

  If you have a specific DLCI you want this traffic to use, enter it here. If none is defined, an available route will be found via an all routes broadcast.
  Range: 16 -- 1023

Connect Type

  This parameter determines whether or not the PU is originating or answering the call.
  Range: Originate or Answer

Advanced

  Click on this button to define the PUs parallel and alternate routes.