#

# EDITOR HOME

# NETWORK PORT

# S-FRAP 3.0 Application Parameters

#### Application Type

#### Circuit Identifier

#### Operation Mode

#### Performance Buffer

#### Tx Timing

#### Application Type

  Defines the type of service provided on the attached network line.
  Range: Dedicated(CBO), Frame Relay(HDLC)

#### Cut-Thru Timeout (min)

  Defines the timer value used to automatically terminate the cut-through state and restore the unit to the configured operating mode. This timer has no effect if the switch on the unit's front panel, is set to the Off position (cut-through state)
  Range: 0 ~ 1440 seconds

#### Circuit Identifier

  Defines the network circuit identifier of the carrier service provider.
  Range: 0 ~ 30 alpha-numeric characters

#### Performance Buffer

  Range: 0 ~ 512.

#### Tx Timing

  Defines the mode of Transmit Timing used.
  Range: Loop1, Loop2, or From Rx Clock

#### Operation Mode

  Defines the operation mode used.
  Range: Tap or In band