MSS 1.1  PTF 8                                          Feb. 25,1999
        PTF 8 is a cumulative PTF, it includes all fixes from PTF 1 to 7
        This PTF is a replacement for all previous PTFs and should be
        installed on the MSS and 8210 to keep the product current.
        PTF 8 does NOT require 64 Meg of RAM in the hardware.
 
-------------------------------------------------------------------------
Attached below is a list of fixes included in MSS 1.1 PTF 8
 
 
NA04021 BugHlt on Login if enter key held down and excessive CR put in
        buffer.
 
IR39000 Change to SAAL control frame transmit priority to insure LEC
        maintains stability and does not test back into the network
 
IR38736 T6 event list all can cause a bughlt if bad Sram record in config
 
IR38735 CIP fix for problem when end station sends data on data direct
before the MSS has completed the circuit establishment, resulted in bughlt
 
IR38706 LE Arp cache error can result in data storage exception.
 
NA03927 SNMP problem when response is large an out of memory bug halt
 
IR38590 BCM cleanup not complete if mac address moves to quickly
 
IR38591 MSS LES/BUS redundant vcc could stop retry after transmit error
 
IR38399 BCM for IP may cause a bughlt if a mac address changes rapidly
        for a specific IP address.
 
IR38075 BOOTP returns wrong gateway error message if an interface has a
        greater (lesser) subnet mask.
 
NA04021 TCP bughlt when using MSS to telnet from, if carriage return
        is last char. in buffer, adding LF would be out of range.
 
IR38452 MAC filter caching can cause MCF filters to not filter correctly
        this apar will disable mac filter caching.
 