
Patch IT453P2.ZIP

This patch corrects some issues associated with the Dial-Out/In 
function of the 8235-I40.  You MUST have the IBM 8235 Management 
Facility version 4.5 already installed before installing this patch.


Procedure for applying patch:


*Note:     If the patch arrives on two 1.44 MG floppy disks,
	   insert the second disk into your floppy drive and 
	   then unzip the files to your harddrive on the machine
	   on which the 8235 Management Facilty resides. This will
	   create the zip files which are referenced below. 	

	1. Copy the zip file, it453p2.zip for Token-Ring  or 
		ie453p2.zip for Ethernet, to the directory where the 
		Management Facility is installed (the default is 
		C:\IBM8235).


	2. Unzip the file in that directory.  When you unzip the file,
		it should prompt you to overwrite a file called
		cards.ini.  Overwrite this file.


	3. Save the configuration and userlist on the 8235-I40.


	4. Do a Clear & Download or IP Auto Download, to load
		the new microcode to the 8235-I40.

	*Note: For IP Auto Download users only, the sbootp.ini will 
	have to	be changed to reflect the above image (ie. IT453.IMG 
	to IT453P2.IMG) before the update is complete.


	5. Set the configuration and userlist you saved.





You can get complete PKZIP and PKUNZIP package from:

	PKWARE BBS: 414-354-3670
	PKWARE WEB: http://www.pkware.com
	
	IBM BBS:    919-517-0001
	IBM WEB:    http://www.pc.ibm.com
	IBM FTP:    ftp.pcco.ibm.com



*Note: The 2.04G version was used to create the zip file so later
	versions should work.

