Last Minute Updates

This diskette contains last minute updates to the following files:

    BE454.IMG       The image files (object code) for the 8235 DIALs 
		    Server for Ethernet. 

    BE454.PKG       The image and VROM files for the 8235 DIALs 
		    Server for Ethernet. 



To install these updated files, you must first install 8235 Management
Facility Version 4.5 on your workstation.  After you install 8235 
Management Facility, insert the 8235 Management Facility for Ethernet
Corrective Service Diskette Version 4.5 in drive A (or the drive for
your 3.5" diskette drive).  Use the latest PKUNZIP.EXE by PKWARE, Inc 
to pkunzip CSD454E.ZIP to the directory where you have the IBM 8235 
Management Facility installed (typically c:\ibm8235).




You can get complete PKZIP and PKUNZIP package from:

	PKWARE BBS: 414-354-3670
	PKWARE WEB: http://www.pkware.com
	
	IBM BBS:    919-517-0001
	IBM WEB:    http://www.pc.ibm.com
	IBM FTP:    ftp.pcco.ibm.com



*Note: The 2.04G version was used to create the zip file so anything 
	newer should work.

*Note: For IP Auto Download users only, the sbootp.ini will have to
	be changed to reflect the above image (ie. BE453.IMG to 
	BE454.IMG) before the update is complete.
