**********************  IBM Unclassified Use ***************************
*
*       LAN NETWORK MANAGER FOR OS/2 V2.0, PTF UR47343
*
* This is PTF UR47343, the current PTF for the Japanese version
* of LNM 2.0 Tier 1, Tier 2 and/or Tier 3. See the FIXES.DAT file
* on the first disk for a list of problems fixed with this driver.
* Finally, please read the READ.ME file on disk 1 for the latest
* information concerning this product.
*
* To create a new images, download the files as binary and run
* LOADDSKF LNMPTFJx.DSK A:
*
* To install, insert the first diskette and type a:install.
*   Select to Upgrade installed components.
*   After this completes, if you wish to install Hub Management,
*      Select Install additional components
* Do NOT select Delete/Reinstall!!!!
*   --If you select this option, you will have to reinstall from
*     your GA diskettes.
*
* NOTE-You may not be prompted to use all diskettes depending on
*      what installation options you select and what components
*      you have installed.
*
************************************************************************
*
*
    LNMPTFJ1 DSK   * PTF UR47343 Disk 1
    LNMPTFJ2 DSK   * PTF UR47343 Disk 2
    LNMPTFJ3 DSK   * PTF UR47343 Disk 3
    LNMPTFJ4 DSK   * PTF UR47343 Disk 4
    LNMPTFJ5 DSK   * PTF UR47343 Disk 5
