
  =====================================================================
  INES IEEE488.2 GPIB Version 6 
  Release 6112
  Copyright 2003, 2004

  Web: www.inesinc.com www.ines.de
  Support: support@inesinc.com
  =====================================================================

  Supported hardware
    
    GPIB-PCI (12.002.00)
    GPIB-PCMCIA
    GPIB-PCI-XL
    GPIB-PCMCIA-XL (32 bit Cardbus)
    GPIB-PC104
    GPIB-PC	(NEC 7210 C installed)
    GPIB-PC-HS	(iGPIB 7210 1.1 installed)

  Installation Instructions for Windows 2000/XP 
  ( Plug&Play cards, for ISA cards see the file isa.txt )

    (1) If a previous version of INES IEEE488.2 GPIB is installed:
	Remove all previous installations of INES IEEE488.2 GPIB 
	by using <distribution-dir-or-drive>\tools\igclreg.exe 

    (2) Install (all) INES GPIB Plug&Play card(s).

    (3) Reboot your computer. Windows recognizes the new hardware.
        Let the Hardware Wizard search for a driver and choose
	CD-ROM (or the directory containing the download content)
	as source.  This adds the hardware specific software components 
	to your computer.

    (4) After the Hardware Wizard has finished, execute setup.exe from
        the installation CD-ROM (or the directory containing the download 
	content) and follow the instructions of the installation program. 
	This adds the generic software components to your computer.

  Installation Instructions for Linux

    see the distributions <linux> subdirectory 

  
