NOTE: 
MD/SMD and SRO should  follow MAS and not RVP Footprint

There may be differences since the RVP may use more pins/types and/or align to socket placement. The MAS is correct for what we recommend land patterns to be manufactured as.
The basic RVP symbol elements though should match the MAS (size, position), but the way etch and connectivity is done can alter pad types.