<?xml version="1.0" encoding="utf-8"?>
<?xml-stylesheet href="ya283.css" type="text/css"?>
<jvcsm COLUMN="2" NEWCOL="0" NEWPAGE="1" PAGESIZE="SINGLE" MODULE="1" ORIENT="PORT" xmlns:HTML="http://www.w3.org/Profiles/XHTML-transitional"><CVR><PCTGR>FLAT COLOUR TELEVISION</PCTGR>
<MNO>No.YA283</MNO>
<ISSUEY>2005/10</ISSUEY>
<ISSUEM>10</ISSUEM>
<MNAME>AV-29M315/V, AV-29M335/V, <BR></BR>
AV-29M315/B, AV-29M515/B, <BR></BR>AV-29M535/B, AV-29V315/V</MNAME></CVR>
<TEXT><TI1 COLUMN="2" NEWCOL="0" NEWPAGE="1" PAGESIZE="SINGLE" MODULE="1" ORIENT="PORT"><HTML:a name="TITLE0"></HTML:a>
<TTL ID="W1114086">1 <HTML:a name="W1114086"></HTML:a>PRECAUTION</TTL>
<TI2 COLUMN="2" NEWCOL="0" NEWPAGE="0" PAGESIZE="SINGLE" MODULE="1" ORIENT="PORT"><HTML:a name="TITLE0-0"></HTML:a>
<TTL>1.1 SAFETY PRECAUTIONS</TTL>
<OL COLUMN="1" NEWCOL="0" NEWPAGE="0"><LI><P COLUMN="1" NEWCOL="0" NEWPAGE="0">The design of this product contains special hardware, many circuits and components specially for safety purposes. For continued protection, no changes should be made to the original design unless authorized in writing by the manufacturer.
Replacement parts must be identical to those used in the original circuits. Service should be performed by qualified personnel only.</P></LI>
<LI><P COLUMN="1" NEWCOL="0" NEWPAGE="0">Alterations of the design or circuitry of the products should not be made. Any design alterations or additions will void the manufacturer's warranty and will further relieve the manufacturer of responsibility for personal injury or property
damage resulting therefrom.</P></LI>
<LI><P COLUMN="1" NEWCOL="0" NEWPAGE="0">Many electrical and mechanical parts in the products have special safety-related characteristics. These characteristics are often not evident from visual inspection nor can the protection afforded by them necessarily be obtained by using replacement
components rated for higher voltage, wattage, etc. Replacement parts which have these special safety characteristics are identified in the parts list of Service manual. <EMP>Electrical components having such features are identified by shading on the schematics
and by ( <GRAPHIC LOC="graphic1" SIZEX="2.963MM" SIZEY="2.625MM" UNIT="mm" HALIGN="CENTER" VALIGN="PAGE" ALIGN="ACENTER" BASELINE="0.000MM" GAP="6.00" ROTATE="0" OFFSETTOP="0.000MM" OFFSETLEFT="0.000MM" IMPSIZE="2.963MM 2.625MM" POSITION="ATINSERTIONPOINT"></GRAPHIC>
<HTML:img src="kigo001.png" width="9" height="8"/>
 ) on the
parts list in Service manual</EMP>. The use of a substitute replacement which does not have the same safety characteristics as the recommended replacement part shown in the parts list of Service manual may cause shock, fire, or other hazards.</P></LI>
<LI><P COLUMN="1" NEWCOL="0" NEWPAGE="0"><EMP>Don't short between the LIVE side ground and ISOLATED (NEUTRAL) side ground or EARTH side ground when repairing.</EMP>
 <BR></BR>
Some model's power circuit is partly different in the GND. The difference of the GND is shown by
the LIVE : ( <GRAPHIC LOC="graphic2" SIZEX="2.540MM" SIZEY="2.117MM" UNIT="mm" HALIGN="CENTER" VALIGN="PAGE" ALIGN="ACENTER" BASELINE="0.000MM" GAP="6.00" ROTATE="0" OFFSETTOP="0.000MM" OFFSETLEFT="0.000MM" IMPSIZE="2.540MM 2.117MM" POSITION="ATINSERTIONPOINT"></GRAPHIC>
<HTML:img src="kigo031.png" width="8" height="6"/>
 ) side GND,
the ISOLATED (NEUTRAL) : ( <GRAPHIC LOC="graphic3" SIZEX="3.133MM" SIZEY="2.879MM" UNIT="mm" HALIGN="CENTER" VALIGN="PAGE" ALIGN="ACENTER" BASELINE="0.000MM" GAP="6.00" ROTATE="0" OFFSETTOP="0.000MM" OFFSETLEFT="0.000MM" IMPSIZE="3.133MM 2.879MM" POSITION="ATINSERTIONPOINT"></GRAPHIC>
<HTML:img src="kigo041.png" width="9" height="9"/>
 )
side GND and EARTH : ( <GRAPHIC LOC="graphic4" SIZEX="2.794MM" SIZEY="2.794MM" UNIT="mm" HALIGN="CENTER" VALIGN="PAGE" ALIGN="ACENTER" BASELINE="0.000MM" GAP="6.00" ROTATE="0" OFFSETTOP="0.000MM" OFFSETLEFT="0.000MM" IMPSIZE="2.794MM 2.794MM" POSITION="ATINSERTIONPOINT"></GRAPHIC>
<HTML:img src="kigo032.png" width="8" height="8"/>
 )
side GND. <BR></BR>Don't short between the LIVE side GND and ISOLATED (NEUTRAL) side GND or EARTH side GND and never measure the LIVE side GND and ISOLATED (NEUTRAL) side GND or EARTH side GND at the same time with a measuring apparatus (oscilloscope
etc.). If above note will not be kept, a fuse or any parts will be broken.</P></LI>
<LI><P COLUMN="1" NEWCOL="0" NEWPAGE="0">If any repair has been made to the chassis, it is recommended that the B1 setting should be checked or adjusted (See B1 POWER SUPPLY check).</P></LI>
<LI><P COLUMN="1" NEWCOL="0" NEWPAGE="0">The high voltage applied to the picture tube must conform with that specified in Service manual. Excessive high voltage can cause an increase in X-Ray emission, arcing and possible component damage, therefore operation under excessive high voltage
conditions should be kept to a minimum, or should be prevented. If severe arcing occurs, remove the AC power immediately and determine the cause by visual inspection (incorrect installation, cracked or melted high voltage harness, poor soldering, etc.).
To maintain the proper minimum level of soft X-Ray emission, components in the high voltage circuitry including the picture tube must be the exact replacements or alternatives approved by the manufacturer of the complete product.</P></LI>
<LI><P COLUMN="1" NEWCOL="0" NEWPAGE="0">Do not check high voltage by drawing an arc. Use a high voltage meter or a high voltage probe with a VTVM. Discharge the picture tube before attempting meter connection, by connecting a clip lead to the ground frame and connecting the other
end of the lead through a 10k<SymbolChar>W</SymbolChar> 2W resistor to the anode button. </P></LI>
<LI><P COLUMN="1" NEWCOL="0" NEWPAGE="0">When service is required, observe the original lead dress. Extra precaution should be given to assure correct lead dress in the high voltage circuit area. Where a short circuit has occurred, those components that indicate evidence of overheating
should be replaced. Always use the manufacturer's replacement components.</P></LI>
<LI><P COLUMN="1" NEWCOL="0" NEWPAGE="0"><EMP>Isolation Check (Safety for Electrical Shock Hazard) </EMP>
<BR></BR>After re-assembling the product, always perform an isolation check on the exposed metal parts of the cabinet (antenna terminals, video/audio input and output terminals, Control
knobs, metal cabinet, screw heads, earphone jack, control shafts, etc.) to be sure the product is safe to operate without danger of electrical shock.</P>
<OL COLUMN="1" NEWCOL="0" NEWPAGE="0"><LI><P COLUMN="1" NEWCOL="0" NEWPAGE="0"><EMP>Dielectric Strength Test</EMP>
 <BR></BR>
The isolation between the AC primary circuit and all metal parts exposed to the user, particularly any exposed metal part having a return path to the chassis should withstand a voltage of 3000V AC
(r.m.s.) for a period of one second. (. . . . Withstand a voltage of 1100V AC (r.m.s.) to an appliance rated up to 120V, and 3000V AC (r.m.s.) to an appliance rated 200V or more, for a period of one second.) <BR></BR>This method of test requires a test
equipment not generally found in the service trade.</P></LI>
<LI><P COLUMN="1" NEWCOL="0" NEWPAGE="0"><EMP>Leakage Current Check</EMP>
 <BR></BR>
Plug the AC line cord directly into the AC outlet (do not use a line isolation transformer during this check.). Using a "Leakage Current Tester", measure the leakage current from each exposed metal part of
the cabinet, particularly any exposed metal part having a return path to the chassis, to a known good earth ground (water pipe, etc.). Any leakage current must not exceed 0.5mA AC (r.m.s.). <BR></BR>However, in tropical area, this must not exceed 0.2mA
AC (r.m.s.). </P>
<TOPIC COLUMN="1" NEWCOL="0" NEWPAGE="0"><TTL>Alternate Check Method</TTL>
<P COLUMN="1" NEWCOL="0" NEWPAGE="0">Plug the AC line cord directly into the AC outlet (do not use a line isolation transformer during this check.). Use an AC voltmeter having 1000<SymbolChar>W</SymbolChar> per volt or more sensitivity in the following manner. Connect a 1500<SymbolChar>W</SymbolChar> 10W resistor
paralleled by a 0.15µF AC-type capacitor between an exposed metal part and a known good earth ground (water pipe, etc.). Measure the AC voltage across the resistor with the AC voltmeter. Move the resistor connection to each exposed metal part, particularly
any exposed metal part having a return path to the chassis, and measure the AC voltage across the resistor. Now, reverse the plug in the AC outlet and repeat each measurement. Any voltage measured must not exceed 0.75V AC (r.m.s.). This corresponds
to 0.5mA AC (r.m.s.). <BR></BR>However, in tropical area, this must not exceed 0.3V AC (r.m.s.). This corresponds to 0.2mA AC (r.m.s.).</P>
<FIG COLUMN="1" NEWCOL="0" NEWPAGE="0" TYPE="INT" ORIENT="PORT"><GRAPHIC LOC="graphic5" SIZEX="69.145MM" SIZEY="37.395MM" UNIT="mm" HALIGN="CENTER" VALIGN="PAGE" ALIGN="ACENTER" GAP="6.00" ROTATE="0" OFFSETTOP="0.000MM" OFFSETLEFT="0.000MM" IMPSIZE="69.145MM 37.395MM" POSITION="BELOWCURRENTLINE"></GRAPHIC>
<HTML:br/>
<HTML:img src="LXM-ST001-001_01.png" class="existsvg"/><!--  width="220" height="119" -->
</FIG></TOPIC></LI></OL></LI></OL></TI2></TI1></TEXT></jvcsm>
