<?xml version="1.0" encoding="utf-8"?>
<?xml-stylesheet href="mb508.css" type="text/css"?>
<jvcsm CNN="2,0,0" PMO="S,1,P" xmlns:HTML="http://www.w3.org/1999/xhtml">
<CVR>
<PCTGR>COMPACT COMPONENT SYSTEM</PCTGR>
<MNO>No.MB508</MNO>
<ISSUEY>2006/06</ISSUEY>
<ISSUEM>6</ISSUEM>
<MNAME>MX-C55J,MX-C55C</MNAME>
</CVR>
<TEXT><TI1 CNN="2,0,0" PMO="S,1,P"><HTML:a name="TITLE2"></HTML:a>
<TTL ID="W1081039">3 <HTML:a name="W1081039"></HTML:a>DISASSEMBLY</TTL>
<TI2 CNN="2,0,0" PMO="S,1,P"><HTML:a name="TITLE2-0"></HTML:a>
<TTL>3.1 Main body section</TTL>
<TI3 CNN="2,0,0" MO="1"><TTL>3.1.1 Removing the top cabinet <BR></BR>
(See Figs.<XREF RID="CHDIBJHE" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDIBJHE">1</HTML:a></XREF>
 and <XREF RID="CHDHEAEE" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDHEAEE">2</HTML:a></XREF>)</TTL>
<OL CNN="1,0,0"><LI><P CNN="1,0,0">From the both sides of the main body, remove the six screws <EMP>A</EMP>
 attaching the top cabinet. (See Fig.<XREF RID="CHDIBJHE" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDIBJHE">1</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">From the back side of the main body, remove the three screws <EMP>B</EMP>
 attaching the top cabinet. (See Fig.<XREF RID="CHDHEAEE" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDHEAEE">2</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">Take out the top cabinet from the main body while lifting the rear section of the top cabinet in the direction of the arrow. (See Fig.<XREF RID="CHDIBJHE" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDIBJHE">1</HTML:a></XREF>.)</P></LI></OL></TI3>
<TI3 CNN="1,0,0" MO="1"><TTL>3.1.2 Removing the CD deck assembly <BR></BR>
(See Figs.<XREF RID="CHDHEAEE" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDHEAEE">2</HTML:a></XREF>
 to <XREF RID="CHDCAJEB" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDCAJEB">4</HTML:a></XREF>)</TTL>
<UL CNN="1,0,0"><LI><P CNN="1,0,0">Remove the top cabinet.</P></LI></UL>
<OL CNN="1,0,0"><LI><P CNN="1,0,0">From the back side of the main body, remove the two screws <EMP>B</EMP>
 attaching the CD deck assembly to the rear cabinet. (See Fig.<XREF RID="CHDHEAEE" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDHEAEE">2</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">From the bottom side of the CD deck assembly, turn the gear cam in the direction of the arrow and draw the tray disc out of the CD deck assembly in the direction of the arrow 1. (See Figs.<XREF RID="CHDEBJFG" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDEBJFG">3</HTML:a></XREF>
 and <XREF RID="CHDCAJEB" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDCAJEB">4</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">Remove the CD door from the tray disc in the direction of the arrow 2. (See Fig.<XREF RID="CHDCAJEB" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDCAJEB">4</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">From the left side of the main body, disconnect the wire from the connector <SYMBOL>CN103</SYMBOL>
 on the main AMP board. (See Fig.<XREF RID="CHDCAJEB" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDCAJEB">4</HTML:a></XREF>)</P></LI>
<LI><P CNN="1,0,0">Disconnect the card wire from the connector <SYMBOL>CW105</SYMBOL>
 on the CD board. (See Fig.<XREF RID="CHDCAJEB" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDCAJEB">4</HTML:a></XREF>)</P></LI>
<LI><P CNN="1,0,0">From the both sides of the main body, remove the two screws <EMP>D</EMP>
 and then take out the CD deck assembly from the main body. (See Fig.<XREF RID="CHDCAJEB" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDCAJEB">4</HTML:a></XREF>.)</P></LI></OL>
<FIG CNN="1,0,0" TYPE="INT" OE="PORT"><CAP ID="CHDIBJHE">Fig. <HTML:a name="CHDIBJHE"></HTML:a>1</CAP>
<!-- GRAPHIC LOC="graphic7" SIZEX="66.675MM" SIZEY="62.795MM" GRATT="6.0" IMPSIZE="66.675MM 62.795MM" GP="L" / -->
<HTML:br/>
<HTML:img src="mb508_3001.png" class="existsvg"/><!--  width="212" height="200" -->
</FIG>
<FIG CNN="1,0,0" TYPE="INT" OE="PORT"><CAP ID="CHDHEAEE">Fig. <HTML:a name="CHDHEAEE"></HTML:a>2</CAP>
<!-- GRAPHIC LOC="graphic8" SIZEX="60.325MM" SIZEY="67.028MM" GRATT="6.0" IMPSIZE="60.325MM 67.028MM" GP="L" / -->
<HTML:br/>
<HTML:img src="mb508_3002.png" class="existsvg"/><!--  width="192" height="213" -->
</FIG>
<FIG CNN="1,0,0" TYPE="INT" OE="PORT"><CAP ID="CHDEBJFG">Fig. <HTML:a name="CHDEBJFG"></HTML:a>3</CAP>
<!-- GRAPHIC LOC="graphic9" SIZEX="59.620MM" SIZEY="70.909MM" GRATT="6.0" IMPSIZE="59.620MM 70.909MM" GP="L" / -->
<HTML:br/>
<HTML:img src="mb508_3003.png" class="existsvg"/><!--  width="190" height="226" -->
</FIG>
<FIG CNN="1,0,0" TYPE="INT" OE="PORT"><CAP ID="CHDCAJEB">Fig. <HTML:a name="CHDCAJEB"></HTML:a>4</CAP>
<!-- GRAPHIC LOC="graphic10" SIZEX="75.142MM" SIZEY="64.559MM" GRATT="6.0" IMPSIZE="75.142MM 64.559MM" GP="L" / -->
<HTML:br/>
<HTML:img src="mb508_3004.png" class="existsvg"/><!--  width="239" height="205" -->
</FIG></TI3>
<TI3 CNN="2,0,1" MO="1"><TTL>3.1.3 Removing the main AMP board <BR></BR>
(See Figs.<XREF RID="CHDDAAFA" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDDAAFA">5</HTML:a></XREF>
 to <XREF RID="CHDFIABC" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDFIABC">7</HTML:a></XREF>)</TTL>
<UL CNN="1,0,0"><LI><P CNN="1,0,0">Remove the top cabinet and CD deck assembly.</P></LI></UL>
<OL CNN="1,0,0"><LI><P CNN="1,0,0">From the right side of the main body, remove the screw <EMP>E</EMP>
 attaching the main AMP board to the main body. (See Fig.<XREF RID="CHDDAAFA" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDDAAFA">5</HTML:a></XREF>)</P></LI>
<LI><P CNN="1,0,0">From the top side of the main body, disconnect the wire from the connector <SYMBOL>CN108</SYMBOL>
 on the main AMP board. (See Fig.<XREF RID="CHDFFFIA" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDFFFIA">6</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">Disconnect the card wire from the connector <SYMBOL>CN101</SYMBOL>
 on the main AMP board. (See Fig.<XREF RID="CHDFFFIA" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDFFFIA">6</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">Disconnect the wire from the connector <SYMBOL>CN102</SYMBOL>
 on the main AMP board. (See Fig.<XREF RID="CHDFFFIA" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDFFFIA">6</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">Disconnect the wires from the connectors (<SYMBOL>SMCN01</SYMBOL>
, <SYMBOL>SMCN02</SYMBOL>
) on the SMPS board. (See Fig.<XREF RID="CHDFFFIA" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDFFFIA">6</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">From the back side of the main body, remove the three screws <EMP>G</EMP>
 attaching the main AMP board to the rear cabinet. (See Fig.<XREF RID="CHDFIABC" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDFIABC">7</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">Take out the main AMP board from the bottom cabinet.</P></LI></OL></TI3>
<TI3 CNN="1,0,0" MO="1"><TTL>3.1.4 Removing the SMPS board and rear cabinet <BR></BR>
(See Figs.<XREF RID="CHDFFFIA" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDFFFIA">6</HTML:a></XREF>
 to <XREF RID="CHDIBJJD" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDIBJJD">8</HTML:a></XREF>)</TTL>
<UL CNN="1,0,0"><LI><P CNN="1,0,0">Remove the top cabinet, CD deck assembly and main AMP board.</P></LI></UL>
<OL CNN="1,0,0"><LI><P CNN="1,0,0">From the top side of the main body, remove the screw <EMP>F</EMP>
 attaching the earth wire on the bottom cabinet. (See Fig.<XREF RID="CHDFFFIA" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDFFFIA">6</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">From the back side of the main body, remove the three screws <EMP>H</EMP>
 attaching the rear cabinet. (See Fig.<XREF RID="CHDFIABC" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDFIABC">7</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">Remove the sections <EMP>a</EMP>
 toward this side and take out the rear cabinet. (See Fig.<XREF RID="CHDFIABC" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDFIABC">7</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">From the inside of the rear cabinet, remove the four screws <EMP>M</EMP>
 attaching the SMPS board. (See Fig.<XREF RID="CHDIBJJD" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDIBJJD">8</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">Release the claw <EMP>b</EMP>
 and take out the SMPS board from the rear cabinet assembly. (See Fig.<XREF RID="CHDIBJJD" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDIBJJD">8</HTML:a></XREF>.)</P></LI></OL></TI3>
<TI3 CNN="1,0,0" MO="1"><TTL>3.1.5 Removing the fan motor <BR></BR>
(See Figs.<XREF RID="CHDFIABC" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDFIABC">7</HTML:a></XREF>
 and <XREF RID="CHDIBJJD" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDIBJJD">8</HTML:a></XREF>)</TTL>
<UL CNN="1,0,0"><LI><P CNN="1,0,0">Remove the top cabinet, CD deck assembly and main AMP board.</P></LI></UL>
<OL CNN="1,0,0"><LI><P CNN="1,0,0">From the back side of the main body, remove the two screws <EMP>K</EMP>
 attaching the fan motor to the rear cabinet. (See Fig.<XREF RID="CHDFIABC" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDFIABC">7</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">Take out the fan motor from the rear cabinet. (See Fig.<XREF RID="CHDIBJJD" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDIBJJD">8</HTML:a></XREF>.)</P></LI></OL>
<FIG CNN="1,0,0" TYPE="INT" OE="PORT"><CAP ID="CHDDAAFA">Fig. <HTML:a name="CHDDAAFA"></HTML:a>5</CAP>
<!-- GRAPHIC LOC="graphic11" SIZEX="61.384MM" SIZEY="73.025MM" GRATT="6.0" IMPSIZE="61.384MM 73.025MM" GP="L" / -->
<HTML:br/>
<HTML:img src="mb508_3005.png" class="existsvg"/><!--  width="195" height="233" -->
</FIG>
<FIG CNN="1,0,0" TYPE="INT" OE="PORT"><CAP ID="CHDFFFIA">Fig. <HTML:a name="CHDFFFIA"></HTML:a>6</CAP>
<!-- GRAPHIC LOC="graphic12" SIZEX="78.317MM" SIZEY="69.145MM" GRATT="6.0" IMPSIZE="78.317MM 69.145MM" GP="L" / -->
<HTML:br/>
<HTML:img src="mb508_3006.png" class="existsvg"/><!--  width="250" height="220" -->
</FIG>
<FIG CNN="1,0,0" TYPE="INT" OE="PORT"><CAP ID="CHDFIABC">Fig. <HTML:a name="CHDFIABC"></HTML:a>7</CAP>
<!-- GRAPHIC LOC="graphic13" SIZEX="71.261MM" SIZEY="72.320MM" GRATT="6.0" IMPSIZE="71.261MM 72.320MM" GP="L" / -->
<HTML:br/>
<HTML:img src="mb508_3007.png" class="existsvg"/><!--  width="227" height="230" -->
</FIG>
<FIG CNN="1,0,0" TYPE="INT" OE="PORT"><CAP ID="CHDIBJJD">Fig. <HTML:a name="CHDIBJJD"></HTML:a>8</CAP>
<!-- GRAPHIC LOC="graphic14" SIZEX="72.320MM" SIZEY="80.434MM" GRATT="6.0" IMPSIZE="72.320MM 80.434MM" GP="L" / -->
<HTML:br/>
<HTML:img src="mb508_3008.png" class="existsvg"/><!--  width="230" height="256" -->
</FIG></TI3>
<TI3 CNN="2,0,1" MO="1"><TTL>3.1.6 Removing the front cabinet assembly <BR></BR>
(See Figs.<XREF RID="CHDDGHAG" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDDGHAG">9</HTML:a></XREF>
 to <XREF RID="CHDGHDID" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDGHDID">11</HTML:a></XREF>)</TTL>
<UL CNN="1,0,0"><LI><P CNN="1,0,0">Remove the top cabinet and CD deck assembly.</P></LI></UL>
<OL CNN="1,0,0"><LI><P CNN="1,0,0">From the top side of the main body, remove the screw <EMP>N</EMP>
 attaching the earth wire on the bottom cabinet. (See Fig.<XREF RID="CHDDGHAG" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDDGHAG">9</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">Disconnect the card wire from the connector <SYMBOL>CN101</SYMBOL>
 on the main AMP board. (See Fig.<XREF RID="CHDGEJDG" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDGEJDG">10</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">Disconnect the wire from the connector <SYMBOL>CN102</SYMBOL>
 on the main AMP board. (See Fig.<XREF RID="CHDGEJDG" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDGEJDG">10</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">From the both sides of the main body, remove the two screws <EMP>P</EMP>
 attaching the front cabinet assembly. (See Fig.<XREF RID="CHDGHDID" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDGHDID">11</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">From the both and bottom sides of the main body, release the joints (<EMP>c</EMP>
, <EMP>d</EMP>
) and then take out the front cabinet assembly from the main body in the direction of the arrow. (See Figs.<XREF RID="CHDGHDID" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDGHDID">11</HTML:a></XREF>.)</P></LI></OL>
<FIG CNN="1,0,0" TYPE="INT" OE="PORT"><CAP ID="CHDDGHAG">Fig. <HTML:a name="CHDDGHAG"></HTML:a>9</CAP>
<!-- GRAPHIC LOC="graphic15" SIZEX="60.678MM" SIZEY="71.261MM" GRATT="6.0" IMPSIZE="60.678MM 71.261MM" GP="L" / -->
<HTML:br/>
<HTML:img src="mb508_3009.png" class="existsvg"/><!--  width="193" height="227" -->
</FIG>
<FIG CNN="1,0,0" TYPE="INT" OE="PORT"><CAP ID="CHDGEJDG">Fig. <HTML:a name="CHDGEJDG"></HTML:a>10</CAP>
<!-- GRAPHIC LOC="graphic16" SIZEX="78.670MM" SIZEY="53.270MM" GRATT="6.0" IMPSIZE="78.670MM 53.270MM" GP="L" / -->
<HTML:br/>
<HTML:img src="mb508_3010.png" class="existsvg"/><!--  width="251" height="169" -->
</FIG>
<FIG CNN="1,0,0" TYPE="INT" OE="PORT"><CAP ID="CHDGHDID">Fig. <HTML:a name="CHDGHDID"></HTML:a>11</CAP>
<!-- GRAPHIC LOC="graphic17" SIZEX="75.142MM" SIZEY="80.081MM" GRATT="6.0" IMPSIZE="75.142MM 80.081MM" GP="L" / -->
<HTML:br/>
<HTML:img src="mb508_3011.png" class="existsvg"/><!--  width="239" height="255" -->
</FIG></TI3>
<TI3 CNN="2,0,1" MO="1"><TTL>3.1.7 Removing the VFD board <BR></BR>
(See Figs.<XREF RID="CHDIDJCD" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDIDJCD">12</HTML:a></XREF>
 and <XREF RID="CHDGJBID" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDGJBID">13</HTML:a></XREF>)</TTL>
<UL CNN="1,0,0"><LI><P CNN="1,0,0">Remove the top cabinet, CD deck assembly and front cabinet assembly.</P></LI></UL>
<OL CNN="1,0,0"><LI><P CNN="1,0,0">From the front side of the front cabinet assembly, pull out the two knobs. (See Fig.<XREF RID="CHDIDJCD" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDIDJCD">12</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">From the inside of the front cabinet assembly, remove the seven screws <EMP>Q</EMP>
 attaching the VFD board. (See Fig.<XREF RID="CHDGJBID" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDGJBID">13</HTML:a></XREF>.)</P></LI>
<LI><P CNN="1,0,0">Take out the VFD board from the front cabinet assembly and then disconnect the wires from the connectors (<SYMBOL>UW101</SYMBOL>
, <SYMBOL>UW201</SYMBOL>
, <SYMBOL>FW102</SYMBOL>
, <SYMBOL>FW104</SYMBOL>
) on the VFD board. . (See Fig.<XREF RID="CHDGJBID" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDGJBID">13</HTML:a></XREF>.)</P></LI></OL></TI3>
<TI3 CNN="1,0,0" MO="1"><TTL>3.1.8 Removing the front board <BR></BR>
(See Fig.<XREF RID="CHDIDJCD" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDIDJCD">12</HTML:a></XREF>)</TTL>
<UL CNN="1,0,0"><LI><P CNN="1,0,0">Remove the top cabinet, CD deck assembly, front cabinet assembly and VFD board.</P></LI></UL>
<OL CNN="1,0,0"><LI><P CNN="1,0,0">From the inside of the front cabinet assembly, remove the four screws <EMP>R</EMP> attaching the front board.</P></LI>
<LI><P CNN="1,0,0">Take out the front board from the front cabinet assembly.</P></LI></OL>
<FIG CNN="1,0,0" TYPE="INT" OE="PORT"><CAP ID="CHDIDJCD">Fig. <HTML:a name="CHDIDJCD"></HTML:a>12</CAP>
<!-- GRAPHIC LOC="graphic18" SIZEX="66.323MM" SIZEY="76.553MM" GRATT="6.0" IMPSIZE="66.323MM 76.553MM" GP="L" / -->
<HTML:br/>
<HTML:img src="mb508_3012.png" class="existsvg"/><!--  width="211" height="244" -->
</FIG>
<FIG CNN="1,0,0" TYPE="INT" OE="PORT"><CAP ID="CHDGJBID">Fig. <HTML:a name="CHDGJBID"></HTML:a>13</CAP>
<!-- GRAPHIC LOC="graphic19" SIZEX="81.492MM" SIZEY="79.023MM" GRATT="6.0" IMPSIZE="81.492MM 79.023MM" GP="L" / -->
<HTML:br/>
<HTML:img src="mb508_3013.png" class="existsvg"/><!--  width="260" height="252" -->
</FIG></TI3>
<TI3 CNN="2,0,1" MO="1"><TTL>3.1.9 Removing the USB board <BR></BR>
(See Fig.<XREF RID="CHDBDICJ" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDBDICJ">14</HTML:a></XREF>)</TTL>
<UL CNN="1,0,0"><LI><P CNN="1,0,0">Remove the top cabinet, CD deck assembly, front cabinet assembly, Knobs and VFD board.</P></LI></UL>
<OL CNN="1,0,0"><LI><P CNN="1,0,0">From the inside of the front cabinet assembly, remove the three screws <EMP>S</EMP> attaching the USB board.</P></LI>
<LI><P CNN="1,0,0">Take out the USB board from the front cabinet assembly.</P></LI></OL></TI3>
<TI3 CNN="1,0,0" MO="1"><TTL>3.1.10 Removing the LED1 board, LED2 board and LED3 board <BR></BR>
(See Fig.<XREF RID="CHDBDICJ" TYPE="FIG" HYTIME="CLINK" HYNAMES="linkend rid"><HTML:a href="mb508_3.xml#CHDBDICJ">14</HTML:a></XREF>)</TTL>
<UL CNN="1,0,0"><LI><P CNN="1,0,0">Remove the top cabinet, CD deck assembly, front cabinet assembly, knobs and VFD board.</P></LI></UL>
<OL CNN="1,0,0"><LI><P CNN="1,0,0">From the inside of the front cabinet assembly, release the claws <EMP>e</EMP> and then take out the LED1 board from the front cabinet assembly.</P></LI>
<LI><P CNN="1,0,0">Remove the screw <EMP>T</EMP> attaching the LED2 board.</P></LI>
<LI><P CNN="1,0,0">Release the claw <EMP>f</EMP> and then take out the LED2 board from the front cabinet assembly.</P></LI>
<LI><P CNN="1,0,0">Take out the LED3 board from the front cabinet assembly.</P></LI></OL>
<FIG CNN="1,0,0" TYPE="INT" OE="PORT"><CAP ID="CHDBDICJ">Fig. <HTML:a name="CHDBDICJ"></HTML:a>14</CAP>
<!-- GRAPHIC LOC="graphic20" SIZEX="76.906MM" SIZEY="75.495MM" GRATT="6.0" IMPSIZE="76.906MM 75.495MM" GP="L" / -->
<HTML:br/>
<HTML:img src="mb508_3014.png" class="existsvg"/><!--  width="245" height="240" -->
</FIG></TI3></TI2></TI1></TEXT>
</jvcsm>
