<?xml version="1.0" encoding="utf-8"?>
<?xml-stylesheet href="mb508_cvr.css" type="text/css"?>
<jvcsm xmlns:HTML="http://www.w3.org/1999/xhtml">
<CVR>
<PCTGR>COMPACT COMPONENT SYSTEM</PCTGR>
<MNO>No.MB508</MNO>
<ISSUEY>2006/06</ISSUEY>
<ISSUEM>6</ISSUEM>
<MNAME>MX-C55J,MX-C55C</MNAME>
<MDLPIC LOC="mdlpic1" SIZEX="171.803MM" SIZEY="102.306MM" GRATT="6" GT="2.117MM" GL="2.117MM" IMPSIZE="167.570MM 98.073MM" GP="L" FRAME="0"></MDLPIC>
<HTML:br/>
<HTML:img src="mb508_0001.png" class="existsvg"/><!--  width="549" height="326" -->
<NOTE CNN="2,0,0"><TTL></TTL>
<P CNN="2,0,0">Lead free solder used in the board (material : Sn-Ag-Cu, melting point : 219 Centigrade)</P></NOTE>
<SPEC>
<HTML:h4>SPECIFICATION</HTML:h4>
<!-- TABLE TE="1" FRAME="ALL" CS="1" RS="1" OE="PORT" CNN="1,0,0" TYPE="OTHER" --><HTML:table frame="box" rules="all"><!-- TGROUP COLS="4" CS="1" RS="1" HA="L" CHAROFF="50" CHAR="" --><!-- COLSPEC CB="1" CN="1" CW="0.972in" --><!-- /COLSPEC -->
<!-- COLSPEC CB="2" CN="2" CW="2.417in" --><!-- /COLSPEC -->
<!-- COLSPEC CB="3" CN="3" CW="1.083in" --><!-- /COLSPEC -->
<!-- COLSPEC CB="4" CN="4" CW="2.822in" --><!-- /COLSPEC -->
<!-- TBODY VA="T" --><!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="1" MRO="5,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="6"><P CNN="1,0,0">Amplifier section</P>
<P CNN="1,0,0">CA-MXC55</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="2" MRO="1,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="2"><P CNN="1,0,0">Output Power</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">SUBWOOFERS</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">170 W per channel, min. RMS, driven into 3 &#x2126; at 63 Hz with no more than 10% total harmonic distortion</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">MAIN SPEAKERS</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">80 W per channel, min. RMS, driven into 6 &#x2126; at 1 kHz with no more than 10% total harmonic distortion</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="2" MRO="1,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="2"><P CNN="1,0,0">Audio input sensitivity/Impedance</P>
<P CNN="1,0,0">(at 1 kHz, measured at MAIN SPEAKERS)</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">AUX</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">400 mV/47 k&#x2126;</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">USB</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">USB Version 1.1</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="2" MRO="1,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="2"><P CNN="1,0,0">Speakers/Impedance</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">Subwoofers</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">3 &#x2126; - 6 &#x2126;</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">Main speakers</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">6 &#x2126; - 16 &#x2126;</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="1" MRO="1,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="2"><P CNN="1,0,0">Tuner</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY NSE="2,3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" colspan="2" rowspan="1"><P CNN="1,0,0">FM tuning range</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">87.50 MHz - 108.00 MHz</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY NSE="2,3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" colspan="2" rowspan="1"><P CNN="1,0,0">AM tuning range</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">530 kHz - 1 710 kHz</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="1" MRO="2,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="3"><P CNN="1,0,0">CD player</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY NSE="2,3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" colspan="2" rowspan="1"><P CNN="1,0,0">CD Capacity</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">3 CDs</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY NSE="2,3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" colspan="2" rowspan="1"><P CNN="1,0,0">Dynamic range</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">85 dB</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY NSE="2,3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" colspan="2" rowspan="1"><P CNN="1,0,0">Signal-to-noise ratio</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">85 dB</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="1" MRO="3,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="4"><P CNN="1,0,0">General</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY NSE="2,3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" colspan="2" rowspan="1"><P CNN="1,0,0">Power requirement</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">AC 120 V , 60 Hz</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY NSE="2,3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" colspan="2" rowspan="1"><P CNN="1,0,0">Power consumption</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">80 W /136 VA (at operation)</P>
<P CNN="1,0,0">7.3 W (on standby)</P>
<P CNN="1,0,0">1 W (in ECO mode)</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY NSE="2,3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" colspan="2" rowspan="1"><P CNN="1,0,0">Dimensions (approx.)</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">270 mm × 317 mm × 402 mm (W/H/D)</P>
<P CNN="1,0,0">(10 11/16 in. × 12 1/2 in. × 15 7/8 in.)</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY NSE="2,3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" colspan="2" rowspan="1"><P CNN="1,0,0">Mass (approx.)</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">5.9 kg (13 lbs)</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="1" MRO="13,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="14"><P CNN="1,0,0">Speaker section</P>
<P CNN="1,0,0">SP-MXC55</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY NSE="2,3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" colspan="2" rowspan="1"><P CNN="1,0,0">Type</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">3-way bass-reflex type</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="2" MRO="2,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="3"><P CNN="1,0,0">Speaker units</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">Subwoofer</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">16 cm (6 5/16 in.) cone ×1</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">Main Woofer</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">10 cm (3 15/16 in.) cone ×1</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">Tweeter</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">5 cm (2 in.) cone ×1</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="2" MRO="1,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="2"><P CNN="1,0,0">Power handling capacity</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">Subwoofer</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">170 W</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">Main speaker</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">80 W</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="2" MRO="1,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="2"><P CNN="1,0,0">Impedance</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">Subwoofer</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">3 &#x2126;</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">Main speaker</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">6 &#x2126;</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="2" MRO="1,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="2"><P CNN="1,0,0">Frequency range</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">Subwoofer</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">30 Hz - 1 000 Hz</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">Main speaker</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">100 Hz - 20 000 Hz</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="2" MRO="1,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="2"><P CNN="1,0,0">Sound pressure level</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">Subwoofer</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">74 dB/W·m</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY CN="3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">Main speaker</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">81 dB/W·m</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="1" --><HTML:tr><!-- ENTRY NSE="2,3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" colspan="2" rowspan="1"><P CNN="1,0,0">Dimensions (approx.)</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">220 mm × 435 mm × 316 mm (W/H/D)</P>
<P CNN="1,0,0">(8 11/16 in. × 17 13/16 in. × 12 1/2 in.)</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW -->
<!-- ROW RS="0" --><HTML:tr><!-- ENTRY NSE="2,3" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" colspan="2" rowspan="1"><P CNN="1,0,0">Mass (approx.)</P></HTML:td><!-- /ENTRY -->
<!-- ENTRY CN="4" MRO="0,0" VHA="T,L" --><HTML:td valign="TOP" align="LEFT" rowspan="1"><P CNN="1,0,0">5.7 kg (12.6 lbs) each</P></HTML:td><!-- /ENTRY --></HTML:tr><!-- /ROW --><!-- /TBODY --><!-- /TGROUP -->
</HTML:table><!-- /TABLE -->
<NOTE CNN="2,0,0"><P CNN="2,0,0">Design and specifications are subject to change without notice.</P></NOTE>
</SPEC>
</CVR>
</jvcsm>
