# DM-81

## DIP METER

### CONTENTS

INTRODUCTION
FEATURES
SPECIFICATIONS
CONTROLS
PRECAUTIONS
APPLICATIONS

1. USE AS A DIP METER
2. OTHER FREQUENCY MEASUREMENTS
3. USE AS A SIGNAL GENERATOR
4. USE AS A CRYSTAL CHECKER AND MARKER GENERATOR
5. USE AS AN ABSORPTION FREQUENCY METER
6. USE AS A FIELD-STRENGTH METER
7. CAPACITANCE AND INDUCTANCE MEASUREMENTS

ADJUSTMENT
PARTS AND SERVICE
PARTS LIST
PRINTED CIRCUIT BOARDS
SCHEMATIC DIAGRAM

### INTRODUCTION

A dip meter is used for adjustment of radio equipment and antennas. The DM-81 is a self-excited oscillator designed for external coupling to the equipment being tested. It features both inductive and capacitive coupling for measuring enclosed coils and toroidal coils (patent pending). This is not possible with conventional testing instruments.

The DM-81 has the following two functions:

1. Inductive coupling (Fig. 1A)

   As shown (Figure 1A), place the coil unit of the dip meter in close proximity to the circuit being measured.

   Adjust the dial. When the dip meter oscillation frequency coincides with the resonant frequency (tuned circuit), oscillating energy is absorbed by the circuit, thus decreasing the oscillation strength.

   This strength is indicated on the meter. The pointer swings back momentarily at the resonant point. Since the meter pointer dips at a tuned point, this instrument is called a dip meter.

2. Capacitive coupling (Fig. 1B)

   This is a special feature of the DM-81 which is not found in any other dip meter. The resonant frequency can be checked simply by touching the capacitance probe to the hot side of the resonant circuit under test, instead of coupling the DM-81's coil and measuring inductively. The frequency is read directly on the dial. See Figure 1B.

   Radio equipment is miniaturized and most coils are enclosed in metal shields. Also, toroidal coils are used in many types of radio equipment, and these coils do not couple to conventional dip meters. The DM-81 has solved this problem.

### FEATURES

1. Measurable frequency range is 700kHz to 25OMHz in seven bands.
2. Ali seven dip meter coils, capacitive probe, earphone and ground clip lead, can be carried within the unit for easy transport and storage.
3. Convenient for both in indoor and outdoor measurements, all solid-state and built-in battery.
4. HC-25U and FT-243 sockets enable use as a crystal checker and marker generator.
5. Amplitude modulation is convenient in aligning receivers when using your DM-81 as a signal generator. Also, when used as the marker generator, amplitude modulation is helpful in precisely calibrating the dial scale even for a receiver having no BFO.
6. An FET and transistor are used in the meter circuit to provide extremely good sensitivity.
7. As an absorption frequency meter, your DM-81 is used both to align transmitters and measure field strength.
8. An earphone plug allows you to monitor transmitted signals.
9. A capacitive probe allows measurements without removing coil shields.
10. It is possible to measure resonant circuit frequencies of toroidal coils. This is not possible with conventional dip meters.

### SPECIFICATIONS

Frequency range: | 700kHz - 250MHz (± 3%) A band 0.7 - 1.6MHz (± 3%) B band 1.5 - 3.6MHz (± 3%) C band 3.0 - 7.4MHz (± 3%) D band 6.9 - 17.5MHz (± 3%) E band 17 - 42MHz (± 3%) F band 41 - 110MHz (± 3%) G band 83 - 250MHz (± 3%)
Modulation: | 1 kHz (sine wave)
Power requirements: | Battery, 9V(006P)
Power consumption: | 9 mA
Semi-conductors: | 1 FET, 3 transistors, 3 diodes
Crystal oscillator element to be used: | HC-25U and FT-243
RF search terminal: | For measuring resonant frequency (capacitive coupling) and checking RF voltage using the supplied probe.
Earphone terminal: | Accepts crystal earphone with 3.5ø plug for monitoring modulated tone.
Dimensions: | 70W x 180H x 45D (mm)
Weight: | Approx. 690g (with accessories)
Accessories: | (1) Coils, A-G bands — 7 pieces (2) Probe — 1 piece (3) Ground clip — 1 piece (4) Crystal earphone — 1 piece (5) Battery, 006P — 1 piece

CAUTION: Do not apply a voltage exceeding 500V (DC + AC peak) to the probe.

### CONTROLS

### PRECAUTIONS

1. Battery and Oscillation Coil Loading

   Taking the coil compartment out, you will find a battery snap connector inside the unit. Fit the snap to the battery. First lay the battery take-out ribbon into the battery holder, then install the battery in place. Place the supplied oscillation coils into the coil compartment and reinstall into the dip meter main body.

   Verify that the battery is serviceable before operating your DM-81. First, turn the POWER switch on. Set the FUNCTION switch to "BATT CHECK". The battery is usable as long as the meter pointer is within the "B.C" zone. A low battery results in weak or unstable oscillation, no oscillation, or frequency error. Replace the battery when weak.

   After use, be sure to turn the POWER switch off. If your DM-81 will not be used for a long period of time, remove the battery. You can easily remove it by pulling the take-out ribbon toward you. Never remove the case screws.

2. Obtaining a Dip Point

   The closer the dip meter is brought to the resonant circuit being checked, the tighter the two are coupled and the deeper the dip point. However, the tuning point becomes so broad that you cannot find the correct resonant frequency. Therefore, it is advisable to move the dip meter a little away from the circuit.

   Note that the A band has a large pull-in effect and therefore the dip point is broad.

3. Measuring Transistor Resonant Circuits

   There is no load problem in measuring vacuum tube resonant circuits. In measuring some resonant (tuning) circuits in transistorized transmitters and receivers, the resonant point cannot always be found by the dipping load. In this event, temporarily disconnect the transistor or operate the given resonant circuit with power on and measure by absorption.

4. Caution in Measuring Transmitters

   Your DM-81 is usable as an absorption frequency meter in measuring transmitter power amplifier tank circuits and similar stages producing high RF energy. In rneasurement, do not abruptly bring the dip meter close to the circuit as the transistors and other parts in the dip meter could be destroyed by excess RF energy. Bring it near the circuit slowly while observing the meter pointer.

5. Caution in Motor Pointer Deflection Change

   The meter pointer may swing slightly as if indicating a dip, This results from a variation in oscillation signal strength while tuning the oscillator variable capacitor. Move the dip meter coil away from the circuit under measurement. The meter pointer will return to full scale for a real dip.

### APPLICATIONS

1. Use as a Dip Meter

   1. Select an oscillation coil covering the desired frequency range.
   2. Install the coil into the socket on top of the dip meter.
   3. Set the FUNCTION switch to "OSC".
   4. Turn the power on.
   5. Turn the SENSITIVITY control until the meter pointer reads at division 0.7. If not to division 0.7, turn the control fully counter-clockwise.
   6. Bring the dip meter coil about 1 cm from the tuned circuit to be measured and slowly turn the dial. The oscillator signal energy will be absorbed by the tuned circuit at the resonant point and the meter will dip abruptly. See Figure 3.

      Note: At first, couple the dip meter coil tightly to the given tuned circuit so that you can easily find the dip point. Then, bring the oscillation coil away until the dip is as narrow as possible, and readjust the dial precisely for an accurate dip point. Now read the correct frequency on the dial.

2. Other Frequency Measurements

   1. Resonant circuit measurement

      A basic measurement with your DM-81 is a frequency check of resonant (tuned) circuits comprised of coils and capacitors. In practice, the dip meter is brought near the coil to be measured as shown in Figure 1A. This illustrates a standard method of resonant frequency measurement.

   2. Use of the capacitive probe

      If a coil to be measured is located in a narrow place and cannot be coupled to the dip meter coil, or if a coil is enclosed in a shield, the probe can be used for accurate measurement. See Figure 4.

      The dip point can be obtained by using the ground clip and probe for frequencies of about 50MHz or lower, and the probe only for about 5OMHz and higher. Toroidal coils can be measured in the same manner. Note that the probe should be connected to the hot side (not the ground side) of the circuit. See connections (a) through (e) in the illustration. The dip point is sometimes critical depending on the circuit or frequency to be measured. An accurate dip point can be obtained by turning the dial slowly.

   3. Antenna resonant frequency measurement

      Any antenna can be regarded as a kind of resonant circuit. Its resonant frequency, therefore, can be measured as illustrated in Figure 5. For measurement, connect a one-turn coil to the feed point at the center of the antenna.

      Couple it with the dip meter coil. Now, you can obtain the antenna resonant frequency in a similar manner to APPLICATIONS Section A. For a vertical antenna or similar antennas for which the other feeder lead is grounded, place the one-turn coil between the antenna and ground.

      Couple the one-turn coil to the dip meter until a dip point is obtained. Then, slowly separate the coil to measure the resonant frequency accurately.

3. Use as a Signal Generator

   Your DM-81 can be used as a signal generator for aligning receivers and similar equipment. Couple the dip meter to the antenna circuit of the receiver as illustrated in Figure 6. The dip meter output carrier will enter the receiver. For aligning an AM receiver, set the FUNCTION switch to "MOD". The receiver will sound a 1kHz tone. Aligning SSB and CW receivers can be achieved by leaving the switch at "OSC" for no modulation. Adjust the capacitor trimmers and inductor cores for maximum receiver "S" meter reading or maximum speaker output.

4. Use as Crystal Checker and Marker Generator

   Your DM-81 car, be modified as a crystal checker by installing a crystal in Place of the oscillation coil (see Figure 7).

   You may use either HC-25U or FT-243 crystals. Also, an HC-6U crystal can be checked if plugged into the FT-243 socket. The oscillation signal strength may vary depending on the type and frequency of the crystal used. Adjust the dial for most stable oscillation.

   In addition, your DM-81 is applicable as a marker generator by installing a marker crystal of 1MHz, 3.5MHz, or the like. The marker generator is useful for calibrating a receiver dial.

5. Use as an Absorption Frequency Meter

   Install an oscillation coil covering the desired frequency range into the socket. Turn the SENSITIVITY control ON and adjust to the minimum meter deflection (just before the OFF position of the control), and set the FUNCTION switch to OSC. You can now use your DM-81 as an absorption frequency meter to receive external energy and indicate its frequency on the meter.

   Figure 8a shows how to measure oscillator frequency. The oscillator coil is coupled with, or brought near, the absorption frequency meter coil. Adjust the dial for maximum meter deflection and read the oscillation frequency. Figure 8b shows the absorption frequency meter coupled to a transmitter tank coil. Its radiated energy can be measured in a similar manner to that of Figure 8a.

   CAUTION: A transmitter power amplifier stage produces high RF energy. The absorption frequency meter should be brought near the tank coil slowly so the meter pointer does not deflect off scale. The earphone ahows you to monitor modulation.

   WARNING: Tube type power amplifiers operate at high RF and DC potentials. Transistorized power amps also produce high RF levels. Observe normal safety procedures for high RF and DC circuits.

6. Use as a Field-Strength Meter

   Your DM-81 can be used to measure the field strength of a transmit antenna. Set up as directed in APPLICATIONS: "Use as Absorption frequency meter". In addition, couple to an antenna as in Figure 9. You can now measure field strength. This application is convenient for transmit antenna matching, radiation pattern adjustments, and similar uses.

7. Capacitance and Inductance Measurements

   The value of an unknown inductor can be obtained in combination with a known capacitor by their resonant frequency, as illustrated in Figure 10. Likewise the value of an unknown capacitor can be calculated. The inductance (L), capacitance (C), and resonant frequency (f) are related as:

   `f = 1 / (2π √(LC))`

   This formula can be rewritten as

   `L = 25,400 / (f² C)`

   `C = 25,400 / (f² L)`

   Where

   L = inductance in µH
   C = capacitance in pF
   f = frequency in MHz

   An inductance or capacitance can easily be calculated by substituting the known values into the above equations.

   The oscillation coils supplied with your DM-81 are useful as the known inductor. Their inductances are

   BAND | INDUCTANCE
   A | 1250 µH
   B | 160 µH
   C | 39 µH
   D | 8.4 µH
   E | 1.2 µH
   F | 0.22 µH
   G | 0.047 µH

   In addition to all these applications, your DM-81 is usable in place of a receiver local oscillator in repairing or alignment, and is effective in other services as well. Also, your DM-81 can serve as a BFO for a receiver without one in receiving a CW or SSB signal. It is useful in a wide variety of situations. By fully understanding the principles of operation your DM-81's capabilities may be extended to other applications.

   For an additional source of general information, the radio amateur's handbook is recommended.

### ADJUSTMENT

VR1: 01 Bias adj.

By using G band, adjust VR1 so that the meter pointer deflection is maximum at 83MHz.

VR2: Meter zero adj.

Adjust VR2 so that the meter deflection is zero when the sensitivity control/power switch is set to just before the OFF position of the control.

VR3: Sensitivity adj.

Optimum position.

VR4: Battery voltage check adj.

Adjust VR4 so that the meter deflection comes to the left edge of the "B.C" zone at 7V when the FUNCTION switch is set to "B.C" position.

### PARTS AND SERVICE

Ordering Spare Parts

When ordering replacement or spare parts for your equipment, be sure to specify the following:

Model and serial number.

Schematic number of the parts.

Printed circuit board number on which the part is located.

Part number and name, if known, and quantity desired.

Service

Should it ever become necessary to return this equipment for repair, pack in its original boxes and packing, and include a full description of the problems involved. Also include your telephone number. You need not return accessory items unless directly related to the service problem. Tag all returned items with your call for easy I.D.

Please mention the model and serial number of your unit in any correspondence, whether phone or written. For future reference, record this information in the space provided on the back cover of this manual.

NOTE:

When claiming warranty service, please include a photocopy of the bill of sale, or other proof of purchase showing the date of sale.

### PARTS LIST

MAIN CHASSIS
Ref. # | Part # | Description
| A01-0859-08 | Case top
| A01-0860-08 | Case bottom
| A09-0506-08 | Coil case
| A10-0471-28 | Chassis
| A29-0502-08 | Top panel
| B20-0918-28 | Dial scale
| B23-0602-08 | Front glass
| B31-0719-08 | Meter
| B40-0772-08 | Name plate (serial #)
| B50-2920-00 | Instruction manual
| C01-0191-08 | Variable capacitor
| E11-0061-08 | Pin jack
| E13-0101-05 | Phone jack
| E18-0207-08 | Crystal socket (FT-243)
| E18-0402-08 | Crystal socket (HC-25U)
| E29-0524-08 | Probe
| E30-1839-08 | Ground clip
| E91-0401-08 | Battery snap
| F20-0619-08 | Insulating plate
| H01-2914-08 | Packing case (inside)
| H12-0533-08 | Pad (formed styrene)
| H19-0507-08 | Accessory box
| H25-0165-08 | Polyethylene bag
| H25-0166-08 | Polyethylene bag
| J19-0477-08 | Battery holder
| J21-1460-08 | Coil mounting hardware
| J21-1461-08 | Variable capacitor mounting hardware
| J25-1279-08 | Printed circuit board
| K29-0254-08 | Push-button
| K29-0255-08 | Dial
| L37-0017-08 | Coil A
| L37-0018-08 | Coil B
| L37-0019-08 | Coil C
| L37-0020-08 | Coil D
| L37-0021-08 | Coil E
| L37-0022-08 | Coil F
| L37-0369-08 | Coil G
|  | Battery 006P 9V
C12 | CC45SL2H050C | Ceramic capacitor 5pF 500WV
C13 | CK45D1H103M | Ceramic capacitor 0.01µF ±20%
R17 | RD14BB2E393J | Carbon resistor 39KΩ ±5% ¼W
VR4 | R12-3513-08 | Semi-fixed resistor 20KΩB
| T18-0052-08 | Earphone
| S32-2001-15 | Slide switch
| X73-1350-00 | AMP unit
| X84-1040-00 | High frequency unit
|  | AMP UNIT (X73-1350-00)
Ref. # | Part # | Description
RESISTOR
R11 | RD14BB2E563J | Carbon resistor 56KΩ ±5% ¼W
R12 | RD14BB2E124J | Carbon resistor 120KΩ ±5% ¼W
R13 | RD14BB2E683J | Carbon resistor 68KΩ ±5% ¼W
R14 | RD14BB2E472J | Carbon resistor 4.7KΩ ±5% ¼W
R15 | RD14BB2E222J | Carbon resistor 2.2KΩ ±5% ¼W
R16 | RD14BB2E561J | Carbon resistor 560Ω ±5% ¼W
VR2 | R12-2506-08 | Semi-fixed resistor 5KΩ
VR3 | R05-3002-08 | Variable resistor (with SW) 1OKΩB
CAPACITOR
C11 | CE04W1C100 | Electrolytic 10µF 16WV
SEMI-CONDUCTOR
|  | FET 2SK19 (GR)
|  | Transistor 2SA719
|  | Zener diode RD-6, 2EB
MISCELLANEOUS
| K29-0256-08 | Knob
| J25-2888-08 | Printed circuit board
HIGH FREQUENCY UNIT (XB4-1040-00)
Ref. # | Part # | Description
RESISTOR
R1 | RD14BB2E562J | Carbon resistor 5.6KΩ ±5% ¼W
R2,6,7 | RD14BB2E124J | Carbon resistor 120KΩ ±5% ¼W
R3 | RD14BB2E222J | Carbon resistor 2.2KΩ ±5% ¼W
R4 | RD14BB2E471J | Carbon resistor 470Ω ±5% ¼W
R5,8 | RD14BB2E103J | Carbon resistor 10KΩ ±5% ¼W
R9 | RD14BB2E472J | Carbon resistor 4.7KΩ ±5% ¼W
R10 | RD14BB2E221J | Carbon resistor 220Ω ±5% ¼W
VR1 | R12-3511-08 | Semi-fixed resistor 20KΩB
CAPACITOR
C1 | CC45SL1H470J | Ceramic 47pF ±5%
C2 | CC45SL1H030C | Ceramic 3pF ±0.25pF
C3 | CC45SL1H010C | Ceramic 1pF ±0.25pF
C4 | CK45D1H103M | Ceramic 0.01µF ±20%
C5,7 | CK45D1H102M | Ceramic 0.001µF ±20%
C6 | CC45SL1H101J | Ceramic 100pF ±5%
C8-10 | CQ92M1H472K | Mylar 4700pF ±10%
C14 | CC45SL1H050C | Ceramic 5pF ±0.25pF
SEMI-CONDUCTOR
Q1 |  | Transistor 2SC1215 (S)
Q2 |  | Transistor 2SC945 (K)
D1,2 |  | Diode 1SS16
MISCELLANEOUS
| L33-0262-08 | Feri-inductor 2mH
| J25-2887-08 | Printed circuit board

### PRINTED CIRCUIT BOARDS

### SCHEMATIC DIAGRAM

Unless otherwise specified, resistors are ¼W and ±5%. Also, the circuit elements may be changed without notice owing to a technical innovation.