CURRENT SENSING terminal

INP:SENS:CURR

Selects channel 1 or 2 of the CURRENT SENSING terminal. Normally, use channel 1.

Command

INPut:SENSing:CURRent {1|2}

INPut:SENSing:CURRent?

Parameter

Value: | 1 | Channel 1 (default)
| 2 | Channel 2

Table 4 shows the setting that is specified when *RST or *RCL is sent.

Response

Returns the selected channel number in the NR1 form in response to INP:SENS:CURR?.