OPERation status register

The OPERation status register is a 16-bit register which contains information about conditions which are part of the KFM2150 normal operation.

Table 9 OPERation status register (STATus:OPERation)

Bit | Bit Weight | Bit Name | Description
0 | 1 | CALibrating | The KFM2150 is in calibration (CAL) mode.
1 | 2 | NOT USED | Not used
2 | 4 | NOT USED | Not used
3 | 8 | NOT USED | Not used
4 | 16 | MEASuring*1 | Indicates whether measurement is in progress on the KFM2150.
5 | 32 | Waiting for TRIGger*2 | Indicates whether the KFM2150 is waiting for a trigger (TRIG).
6 | 64 | NOT USED | Not used
7 | 128 | NOT USED | Not used
8 | 256 | PROTecction | The protection function is activated.
9 | 512 | Soft STart is in progress | Soft STart is in progress Soft start (rising or falling edge) is in progress.
10 | 1024 | NOT USED | Not used
11 | 2048 | NOT USED | Not used
12 | 4096 | NOT USED | Not used
13 | 8192 | NOT USED | Not used
14 | 16384 | NOT USED | Not used
15 | 32768 | NOT USED | Always zero

*1. A summary bit of the STAT:OPER:MEAS register. Further detailed information can be obtained by referring to this register.

*2. A summary bit of the STAT:OPER:TRIG register. Further detailed information can be obtained by referring to this register.

STAT:OPER

Queries the event of the OPERation status register.

A query clears the contents of the register.

Command

STATus:OPERation[:EVENt]?

Response

Returns the event of the OPERation status register in the NR1 form.

STAT:OPER:COND

Queries the condition of the OPERation status register.

A query does not clear the contents of the register.

Command

STATus:OPERation:CONDtion?

Response

Returns the condition of the OPERation status register in the NR1 form.

STAT:OPER:ENAB

Sets the enable register of the OPERation status register.

Command

STATus:OPERation:ENABle <NR1>

STATus:OPERation:ENABle?

Parameter

Value: 0 to 32767

Response

Returns the enable register setting of the OPERation status register in the NR1 form.

STAT:OPER:PTR

Sets the positive transition of the OPERation status register.

Command

STATus:OPERation:PTRansition <NR1>

STATus:OPERation:PTRansition?

Parameter

Value: 0 to 32767

Response

Returns the positive transition of the OPERation status register in the NR1 form.

STAT:OPER:NTR

Sets the negative transition of the OPERation status register.

Messages

STATus:OPERation:NTRansition <NR1>

STATus:OPERation:NTRansition?

Parameter

Value: 0 to 32767

Response

Returns the negative transition of the OPERation status register in the NR1 form.