Sub-system Search

FETCh | READ | MEASure subsystem | INPut subsystem | SENSe subsystem
SOURce subsystem | STATus subsystem | SYSTem subsystemm | TRIGger subsystem
Other commands | IEEE488.2 common commands

FETCh | MEASure subsystem
Queries the measured data.
FETC:IMP FETC:ARR:IMP | Measured value of Impedance measurement (magnitude)
FETC:IMP:RES FETC:ARR:IMP:RES | Measured value of Impedance measurement (resistance)
FETC:IMP:REAC FETC:ARR:IMP:REAC | Measured value of Impedance measurement (reactance)
FETC:IMP:PHAS FETC:ARR:IMP:PHAS | Measured value of Impedance measurement (phase angle)
FETC:VOLT FETC:ARR:VOLT | Measured value of voltage output
FETC:VOLT:CYCL FETC:ARR:VOLT:CYCL | Voltage measurement (Voltage synchronized to the impedance measurement)
FETC:CURR FETC:ARR:CURR | Measured value of current output
FETC:CURR:CYCL FETC:ARR:CURR:CYCL | Current measurement (Current synchronized to the impedance measurement)
Starts the measurement and queries the data.
READ:IMP READ:ARR:IMP | Measured value of Impedance measurement (magnitude)
READ:IMP:RES READ:ARR:IMP:RES | Measured value of Impedance measurement (resistance)
READ:IMP:REAC READ:ARR:IMP:REAC | Measured value of Impedance measurement (reactance)
READ:IMP:PHAS READ:ARR:IMP:PHAS | Measured value of Impedance measurement (phase angle)
READ:VOLT READ:ARR:VOLT | Measured value of voltage output
READ:VOLT:CYCL READ:ARR:VOLT:CYCL | Voltage measurement (Voltage synchronized to the impedance measurement)
READ:CURR READ:ARR:CURR | Measured value of current output
READ:CURR:CYCL READ:ARR:CURR:CYCL | Current measurement (Current synchronized to the impedance measurement)
Resets a portion of the settings to default, starts the measurement, and queries the data.
MEAS:IMP MEAS:ARR:IMP | Measured value of Impedance measurement (magnitude)
MEAS:IMP:RES MEAS:ARR:IMP:RES | Measured value of Impedance measurement (resistance)
MEAS:IMP:REAC MEAS:ARR:IMP:REAC | Measured value of Impedance measurement (reactance)
MEAS:IMP:PHAS MEAS:ARR:IMP:PHAS | Measured value of Impedance measurement (phase angle)
MEAS:VOLT MEAS:ARR:VOLT | Measured value of voltage output
MEAS:VOLT:CYCL MEAS:ARR:VOLT:CYCL | Voltage measurement (Voltage synchronized to the impedance measurement)
MEAS:CURR MEAS:ARR:CURR | Measured value of current output
MEAS:CURR:CYCL MEAS:ARR:CURR:CYCL | Current measurement (Current synchronized to the impedance measurement)

>>TOP

INPut subsystem
INP | Load on/off
INP:PROT:CLE | Alarm clear
INP:SST:FALL | Soft start falling edge
INP:SST:RISE | Soft start rising edge
INP:SST:RTIM | Remaining time
INP:SENS:CURR | CURRENT SENSING channel
INP:SENS:VOLT | VOLTAGE SENSING channel

>>TOP

SENSe subsystem
IMP:CURR:AC | Averaging period of the measured value
IMP:CURR:AC:RAT | Measuring AC current (percentage)
IMP:CURR:AC:FREQ | Measuring frequency
IMP:CURR:PULS:DEPT | Pulse depth (current)
IMP:CURR:PULS:DEPT:RAT | Pulse depth
IMP:CURR:PULS:TRAN | Pulse transition time
IMP:CURR:PULS:WIDT | Pulse width
IMP:AVER:MOV:CLE | Moving average area
IMP:AVER:MOV:COUN | Moving average count
IMP:SAMP:POS | Sampling start position
IMP:SAMP:REG | Sampling region
METH | Measurement method
VOLT:PROT:LOW | Voltage sensing undervoltage protection
VOLT:PROT:LOW:DEL | Voltage sensing undervoltage protection delay time

>>TOP

SOURce subsystem
SOUR:CURR | AC current limit
SOUR:CURR:EXT | External electronic load DC current
SOUR:CURR:RANG | Electronic load DC current range
SOUR:VOLT | Voltage of PLZ-4W Series
SOUR:VOLT:RANG | Voltage range of PLZ-4W Series
SOUR:VOLT:PROT:LOW | Undervoltage protection
SOUR:POW:PROT | PLZ4W OPP activation voltage of the electronic load DC voltage

>>TOP

STATus subsystem
STAT:OPER | Queries the event *1
STAT:OPER:COND | Queries the condition of the register *1
STAT:OPER:ENAB | Enable register *1
STAT:OPER:PTR | Positive transition *1
STAT:OPER:NTR | Negative transition *1
STAT:OPER:MEAS | Queries the event *2
STAT:OPER:MEAS:COND | Queries the condition of the register *2
STAT:OPER:MEAS:ENAB | Enable register *2
STAT:OPER:MEAS:PTR | Positive transition *2
STAT:OPER:MEAS:NTR | Negative transition *2
STAT:OPER:TRIG | Queries the event *3
STAT:OPER:TRIG:COND | Queries the condition of the register *3
STAT:OPER:TRIG:ENAB | Enable register *3
STAT:OPER:TRIG:PTR | Positive transition *3
STAT:OPER:TRIG:NTR | Negative transition *3
STAT:OPER:PROT | Queries the event *4
STAT:OPER:PROT:COND | Queries the condition of the register *4
STAT:OPER:PROT:ENAB | Enable register *4
STAT:OPER:PROT:PTR | Positive transition *4
STAT:OPER:PROT:NTR | Negative transition *4
STAT:PRES | Constructing status data
STAT:QUES | Queries the event *5
STAT:QUES:COND | Queries the condition of the register *5
STAT:QUES:ENAB | Enable register *5
STAT:QUES:PTR | Positive transition *5
STAT:QUES:NTR | Negative transition *5

*1 | OPERation status register
*2 | OPERation:MEASuring status register
*3 | OPERation:TRIGger status register
*4 | OPERation:PROTecting status register
*5 | QUEStionable status register

>>TOP

SYSTem subsystem
SYST:COMM:SER:PACE | Flow conrol condition
SYST:ERR | Reads the error information
SYST:LOC | Go To Local
SYST:REM | Remote Enable
SYST:RWL | Local Lock Out
SYST:VERS | SCPI revision

>>TOP

TRIGger subsystemm
ABOR | Aborts the sequence 1 and 2 operations
INIT | Start the trigger function
INIT:SEQ | Sequence 1: Start the trigger function
INIT:SEQ2 | Sequence 2: Start the trigger function
INIT:SEQ:WAV | Sequence 1: Starts the trigger function while holding the voltage and current waveform data
TRIG:COUN | Sequence 1: Trigger count
TRIG:SOUR | Sequence 1: Trigger-wait status
TRIG:TIM | Sequence 1: Trigger time setting
TRIG:SEQ2:COUN | Sequence 2: Trigger count
TRIG:SEQ2:SOUR | Sequence 2: Trigger-wait status
TRIG:SEQ2:TIM | Sequence 2: Trigger time setting

>>TOP

Other commands
FORM:BORD | Data transmission/recording mode
FORM:PAGE:LENG | Length of the data to be transferred
FORM:PAGE:STAR | Start point of the data to be transferred
TRAC | Voltage waveform data or current waveform data

>>TOP

IEEE488.2 common commands
*CLS | Clears the status data structures.
*ESE | Sets the event status enable register bits.
*ESR | Queries the event status register.
*IDN | Queries the identification string (manufacturer information).
*OPC | Causes the device to generate the operation complete message in the event status register when all pending selected device operations have been finished.
*RCL | Recalls the contents saved to the memory.
*RST | Performs a device reset. Configures the KFM2150 to a known condition independent from the usage history of the device.
*SAV | Saves the current settings to the memory.
*SRE | Sets the service request enable register bits.
*STB | Reads the status byte and master summary status bits.
*TRG | Trigger command
*TST | Since there is no self-test function built into the KFM2150.
*WAI | Prevents the device from executing subsequent commands or queries until the No Operation Pending flag becomes true.

>>TOP