OPERation:MEASuring / OPERation:TRIGger status register

The MEASuring and TRIGger status registers indicate measuring or trigger-wait status of the KFM2150.

Only bits 1 and 2 are used.

Table 10 MEASuring/TRIGger status register (STATus:OPERation:MEASuring/STATus:OPERation:TRIGger)

Bit | Bit Weight | Bit Name | Description
0 | 1 | Not Used | Not Used
1 | 2 | SEQ1 (SEQuence1) | Impedance measurement
2 | 4 | SEQ2 (SEQuence2) | Voltage and current measurement
3 | 8 | Not Used | Not Used
4 | 16 | Not Used | Not Used
5 | 32 | Not Used | Not used
6 | 64 | Not Used | Not used
7 | 128 | Not Used | Not Used
8 | 256 | Not Used | Not Used
9 | 512 | Not Used | Not Used
10 | 1024 | Not Used | Not Used
11 | 2048 | Not Used | Not Used
12 | 4096 | Not Used | Not Used
13 | 8192 | Not Used | Not used
14 | 16384 | Not Used | Not used
15 | 32768 | Not Used | Always zero

STAT:OPER:MEAS / STAT:OPER:TRIG

Queries the event of the MEASuring / TRIGger status register.

A query clears the contents of the register.

Command

STATus:OPERation:MEASuring[:EVENt]?

STATus:OPERation:TRIGger[:EVENt]?

Response

Returns the event of the MEASuring / TRIGger status register in the NR1 form.

STAT:OPER:MEAS:COND / STAT:OPER:TRIG:COND

Queries the condition of the MEASuring / TRIGger status register.

A query does not clear the contents of the register.

Command

STATus:OPERation:MEASuring:CONDtion?

STATus:OPERation:TRIGger:CONDtion?

Response

Returns the condition of the MEASuring / TRIGger status register in the NR1 form.

STAT:OPER:MEAS:ENAB / STAT:OPER:TRIG:ENAB

Sets the enable register of the MEASuring / TRIGger status register.

Command

STATus:OPERation:MEASuring:ENABle <NR1>

STATus:OPERation:MEASuring:ENABle?

STATus:OPERation:TRIGger:ENABle <NR1>

STATus:OPERation:TRIGger:ENABle?

Parameter

Value: 0 to 32767

Response

Returns the enable register setting of the MEASuring / TRIGger status register in the NR1 form.

STAT:OPER:MEAS:PTR / STAT:OPER:TRIG:PTR

Sets the positive transition of the MEASuring / TRIGger status register.

Command

STATus:OPERation:MEASuring:PTRansition <NR1>

STATus:OPERation:MEASuring:PTRansition?

STATus:OPERation:TRIGger:PTRansition <NR1>

STATus:OPERation:TRIGger:PTRansition?

Parameter

Value: 0 to 32767

Response

Returns the positive transition of the MEASuring / TRIGger status register in the NR1 form.

STAT:OPER:MEAS:NTR / STAT:OPER:TRIG:NTR

Sets the negative transition of the MEASuring / TRIGger status register.

Command

STATus:OPERation:MEASuring:NTRansition <NR1>

STATus:OPERation:MEASuring:NTRansition?

STATus:OPERation:TRIGger:NTRansition <NR1>

STATus:OPERation:TRIGger:NTRansition?

Parameter

Value: 0 to 32767

Response

Returns the negative transition of the MEASuring / TRIGger status register in the NR1 form.