OPERation status register

The OPERation status register is a 16-bit register which contains information about conditions which are part of the KFM2151 normal operation.

Table 6 OPERation status register (STATus:OPERation)

Bit | Bit Weight | Bit Name | Description
0 | 1 | NOT USED | Not used
1 | 2 | NOT USED | Not used
2 | 4 | NOT USED | Not used
3 | 8 | NOT USED | Not used
4 | 16 | MEASuring | Indicates whether measurement is in progress on the KFM2151.
5 | 32 | NOT USED | Not used
6 | 64 | NOT USED | Not used
7 | 128 | NOT USED | Not used
8 | 256 | NOT USED | Not used
9 | 512 | NOT USED | Not used
10 | 1024 | NOT USED | Not used
11 | 2048 | NOT USED | Not used
12 | 4096 | NOT USED | Not used
13 | 8192 | NOT USED | Not used
14 | 16384 | NOT USED | Not used
15 | 32768 | NOT USED | Always zero

STAT:OPER

Queries the event of the OPERation status register.

A query clears the contents of the register.

Command

STATus:OPERation[:EVENt]?

Response

Returns the event of the OPERation status register in the <NR1> form.

STAT:OPER:COND

Queries the condition of the OPERation status register.

A query does not clear the contents of the register.

Command

STATus:OPERation:CONDtion?

Response

Returns the condition of the OPERation status register in the <NR1> form.

STAT:OPER:ENAB

Sets the enable register of the OPERation status register.

Command

STATus:OPERation:ENABle <NR1>

STATus:OPERation:ENABle?

Parameter

Value: 0 to 32767

Response

Returns the enable register setting of the OPERation status register in the <NR1> form.

STAT:OPER:PTR

Sets the positive transition of the OPERation status register.

Command

STATus:OPERation:PTRansition <NR1>

STATus:OPERation:PTRansition?

Parameter

Value: 0 to 32767

Response

Returns the positive transition of the OPERation status register in the <NR1> form.

STAT:OPER:NTR

Sets the negative transition of the OPERation status register.

Messages

STATus:OPERation:NTRansition <NR1>

STATus:OPERation:NTRansition?

Parameter

Value: 0 to 32767

Response

Returns the negative transition of the OPERation status register in the <NR1> form.