Voltage measurement

VOLT:PROT:LOW

Sets the activation voltage of the voltage sensing undervoltage protection (SENSE UVP).

Command

[SENSe:]VOLTage[:DC]:PROTection:LOWer {<numeric>|MIN|MAX|DEF}

[SENSe:]VOLTage[:DC]:PROTection:LOWer? [{MIN|MAX]}

Parameter

Value: | -2 to 150 (default: -2)
Unit: | V

Table 4 shows the setting that is specified when *RST , *RCL or MEAS? is sent.

Response

Returns the activation voltage of the voltage sensing undervoltage protection in the NR3 form in response to VOLT:PROT:LOW?.

VOLT:PROT:LOW:DEL

Sets the activation delay time of the voltage sensing undervoltage protection.

Command

[SENSe:]VOLTage[:DC]:PROTection:LOWer:DELay {<numeric>|MIN|MAX|DEF}

[SENSe:]VOLTage[:DC]:PROTection:LOWer:DELay? [{MIN|MAX]}

Parameter

Value: | 0.0 to 10.0 (default: 4.0)
Unit: | S

Table 4 shows the setting that is specified when *RST or *RCL is sent.

Response

Returns the activation delay time of the voltage sensing undervoltage protection in the NR3 form in response to VOLT:PROT:LOW:DEL?.