Interface Setup | GPIB Interface
RS232C Interface | USB Interface

GPIB Interface

GPIB connection

Use a standard IEEE488 cable to connect the KFM2150 to the computer.

Setting the GPIB address

By factory default, the GPIB address is set 3.

The address can be set in the range of 1 to 30.

1. Check that the load is turned off.

2. Press the MENU key.
The MENU screen appears.

3. Press the , , and arrow keys to select Configuration > Interface > TYPE and turn the rotary knob to select GPIB.

4. Press the or arrow key to select Address, and turn the rotary knob to set the address.

5. Press the MENU key.
The MENU screen closes.

6. Turn the POWER switch off and then turn it back on.
The settings are entered.

GPIB function

Table 1 GPIB functions

Function | Subset | Description
Source handshake | SH1 | Complete capability
Acceptor handshake | AH1 | Complete capability
Talker | T6 | Function available
Listener | L4 | Function available
Service request | SR1 | Complete capability
Remote local | RL1 | Complete capability
Parallel poll | PP0 | No capability
Device clear | DC1 | Complete capability
Device trigger | DT1 | Complete capability
Controller | C0 | No capability
Electrical interface | E1 | Open collector driver

Service request

Service request and serial polling functions are implemented.