Overview of Messages | Command Syntax
Parameters | Default settings

Default settings

The settings after an *RST command, *RCL command, MEAS:<meter_fn>? command, and power-on are indicated in Table 4.

| *RCL: | Recalls the contents saved to the memory (0 to 3).
| *RST: | Initializes the settings to their factory default values. However, the contents of the three memories remain unchanged.
| MEAS:<meter_fn>?: | Initializes a portion of the settings to default, starts the measurement, and queries the data.

Table 4 Default settings

Setup Item | Setting | Unit | Function
*RST | *RCL | MEAS?*1 | At power-om
IMP:AVER:MOV:COUNT | 1 | *2 | 1 | *3 | - | Moving average count
IMP:CURR:AC | 0 | *4 | Arms | Measureing AC current
IMP:CURR:AC:RAT | 10 | 10 | % | Measuring AC current (as a percentage of the load current)
IMP:CURR:AC:FREQ | 20 000 | 20 000 | Hz | Measuring frequency
IMP:CURR:PULS:TRAN | 0.01 m | 0.01 m | s | Pulse transition time of the interrupt current
IMP:CURR:PULS:WIDT | 0.01 | 0.01 | s | Pulse width of the interrupt current
IMP:CURR:PULS:DEPT:RAT | 100 | 100 | % | Pulse depth of the interrupt current (ass a percentage of the load current)
IMP:CURR:PULS:DEPT | 0 | 0 | A | Pulse depth of the interrupt current
IMP:SAMP:POS | 0.06 m | 0.06 m | s | Sampling start position
IMP:SAMP:REG | 0.03 m | 0.03 m | s | Sampling range
VOLT:PROT:LOW | -2 | -2 | V | Voltage sensing undervoltage protection
VOLT:PROT:LOW:DEL | 4 | No change | s | Voltage sensing undervoltage protection delay time
METH | ACIM | - | Impedance measurement method ACIM: AC Impedance Method
INP | OFF | No change | OFF | - | Load on/off
INP:SST:RISE | 0 | *2 | *3 | S | Soft start rising edge
INP:SST:FALL | 0 | S | Soft start falling edge
INP:SENS:VOLT | 1 | - | Voltage measurement channel
INP:SENS:CURR | 1 | - | Current measurement channel
SOUR:CURR | 0 | A | PLZ-4W load current
SOUR:CURR:EXT | 0 | A | Current of the external electronic load
SOUR:CURR:RANG | HIGH | - | PLZ-4W load current range
SOUR:VOLT | 0 | V | PLZ-4W voltage
SOUR:VOLT:RANG | HIGH | - | PLZ-4W voltage range
SOUR:VOLT:PROT:LOW | -1 | V | PLZ-4W undervoltage protection
SOUR:POW:PROT | *5 | W | PLZ-4W overpower protection
FORM:BORD | NORM | No change | NORM | - | Data transmission/recording mode NORM:Big Endian
FORM:PAGE:STAR | 0 | 0 | s | Start point of the data to be transferred
FORM:PAGE:LENG | 0.1 | 0.1 | s | Length of the ddata to be transferred
TRIG:COUN TRIG:SEQ2:COUN | 1 | 1 | 1 | - | Trigger count
TRIG:TIM TRIG:SEQ2:TIM | 0.01 | 0.01 | 0.01 | s | Trigger hold off
TRIG:SOUR TRIG:SEQ2:SOUR | IMM | IMM | IMM | - | Trigger source IMM: Immediate

*1. MEAS:<meter_fn>?

*2. Depends on the settings in the memory.

*3. Settings immediately before the power switch was turned off.

*4. Present DC load current setting (SOUR:CURR) *1/10

*5. Depends on the rated load current of the PLZ-4W Series.