OPERation:PROTecting status register

The PROTecting status register indicates information when a protection or limit function is activated.

Table 11 PROTecting status register (STATus:OPERation:PROTecting)

Bit | Bit Weight | Bit Name | Description
0 | 1 | OV (Over Voltage Protection) | Overvoltage protection activated
1 | 2 | UV (Under Voltage protection) | Undervoltage protection activated
2 | 4 | OC (Over Current protection) | Overcurrent protection activated
3 | 8 | OP (Over Power protection) | Overpower protection activated
4 | 16 | OT (Over Temperature protection) | Overtemperature protection activated
5 | 32 | Not Used | Not used
6 | 64 | EXT Problem (External Problem) | Alarm input detected (PLZ-4W)
7 | 128 | REV (Reverse Voltage) | Reverse connection detected
8 | 256 | Not Used | Not used
9 | 512 | Not Used | Not used
10 | 1024 | Not Used | Not used
11 | 2048 | Not Used | Not used
12 | 4096 | Not Used | Not used
13 | 8192 | Not Used | Not used
14 | 16384 | USR (User ALARM Input) | Alarm input detected (KFM2150)
15 | 32768 | Not Used | Always zero

STAT:OPER:PROT

Queries the event of the PROTecting status register.

A query clears the contents of the register.

Command

STATus:OPERation:PROTecting[:EVENt]?

Response

Returns the event of the PROTecting status register in the NR1 form.

STAT:OPER:PROT:COND

Queries the condition of the PROTecting status register.

A query does not clear the contents of the register.

Command

STATus:OPERation:PROTecting:CONDtion?

Response

Returns the condition of the PROTecting status register in the NR1 form.

STAT:OPER:PROT:ENAB

Sets the enable register of the PROTecting status register.

Command

STATus:OPERation:PROTecting:ENABle <NR1>

STATus:OPERation:PROTecting:ENABle?

Parameter

Value: 0 to 32767

Response

Returns the enable register setting of the PROTecting status register in the NR1 form.

STAT:OPER:PROT:PTR

Sets the positive transition of the PROTecting status register.

Command

STATus:OPERation:PROTecting:PTRansition <NR1>

STATus:OPERation:PROTecting:PTRansition?

Parameter

Value: 0 to 32767

Response

Returns the positive transition of the PROTecting status register in the NR1 form.

STAT:OPER:PROT:NTR

Sets the negative transition of the PROTecting status register.

Command

STATus:OPERation:PROTecting:NTRansition <NR1>

STATus:OPERation:PROTecting:NTRansition?

Parameter

Value: 0 to 32767

Response

Returns the negative transition of the PROTecting status register in the NR1 form.