This manual describes the procedure for connecting the interface and the procedure for transmitting commands to the KFM2151 using SCPI commands.

Overview

In addition to using the front panel, the KFM2151 can be controlled remotely using the RS232C interface.

The remote interface complies with IEEE Std 488.2-1992 and SCPI Specification 1999.0.

Use the SCPI commands only after you have understood the SCPI command syntax on the KFM2151.