Function Search

IEEE488.2 common commands | Channel commandd
Releasing the Protection Function | Configuration Function
Measurement Function | Other Commands | Register

IEEE488.2 common commands
| *CLS | Clears the status data structures.
| *ESE | Sets the event status enable register bits.
| *ESR | Queries the event status register.
| *IDN | Queries the identification string (manufacturer information).
| *OPC | Causes the device to generate the operation complete message in the event status register when all pending selected device operations have been finished.
| *RST | Performs a device reset. Configures the KFM2151 to a known condition independent from the usage history of the device.
| *SRE | Sets the service request enable register bits.
| *STB | Reads the status byte and master summary status bits.
| *TRG | Trigger command
| *TST | Since there is no self-test function built into the KFM2151.
| *WAI | Prevents the device from executing subsequent commands or queries until the No Operation Pending flag becomes true.

>>TOP

Channel command
| CHAN:VOLT:TERM | Specify the logical channel for voltage scanning and set the terminal and the scanned source
| CHAN:VOLT:NSEL | Specifies the logical channel for voltage scanning
| CHAN:ROUT:TERM | Specify the logical channel for impedance scanning and set the terminal and the scanned source
| CHAN:ROUT:NSEL | Specify the logical channel for impedance scanning
| VOLT:RANG | Sets the voltage range (the channel specified by CHAN:VOLT:NSEL)
| VOLT:RANG:AUTO | Sets the voltage range to auto (the channel specified by CHAN:VOLT:NSEL)
| VOLT:PROT | Sets the voltage protection (OVP) (the channel specified by CHAN:VOLT:NSEL)
| VOLT:PROT:LOW | Sets the voltage protection (UVP) (the channel specified by CHAN:VOLT:NSEL)

>>TOP

Releasing the Protection Function
| INP:PROT:CLE | Releases the alarm

>>TOP

Configuration Function
| CONF:VOLT | Sets the voltage range, and sets the voltage protecction to default (the channel specified by CHAN:VOLT:NSEL)
| CONF:VOLT:ALL | Sets the voltage range, and sets the voltage protecction to default (all logical channels)
| CONF | Queries the voltage range setting

>>TOP

Measurement Function
| INIT | Start the voltage scanning
| ABOR | Aborts the measurement
| *RST | Sequence 1: Trigger time setting
| FETC / FETC:ARR | Queries the voltage measurement data
| READ / READ:ARR | Performs voltage scanning and queries the voltage measurement data
| MEAS:VOLT / MEAS:ARR:VOLT | Resets the settings to default (the range can be set), performs voltage scanning, and queries the voltage measurement data

>>TOP

Other Commands
| SYST:ERR | Reads the error information
| SYST:VERS | Version of the SCPI specifications to which the KFM2150 conforms
| SYST:FORM:INST:COUN | Queries the number of KFM2151s that are connected

>>TOP

Register
Status byte register
Event status register
OPERation status register
| STAT:OPER | Queries the event
| STAT:OPER:COND | Queries the condition of the register
| STAT:OPER:ENAB | Enable register
| STAT:OPER:NTR | Negative transition
| STAT:OPER:PTR | Positive transition
QUEStionable status register
| STAT:QUES | Queries the event
| STAT:QUES:COND | Queries the condition of the register
| STAT:QUES:CONT:LIST:OVP | Queries the condition of bit 10 (OVP) of the QUEStionable status register
| STAT:QUES:CONT:LIST:UVP | Queries the condition of bit 9 (UVP) of the QUEStionable status register
| STAT:QUES:ENAB | Enable register
| STAT:QUES:NTR | Negative transition
| STAT:QUES:PTR | Positive transition
Preset Status
| STAT:PRES | Constructing status data

>>TOP