Measurement functions of the KFM2150 | Simple measurement procedure (MEASure)
Measurement procedure with flexibility (READ) | Most flexible measurement procedure (INITiate and FETCh)
Measurement using software triggers | Multipoint measurement with specified trigger count
Waveform data retrieval function

Tutorial

This section describes the procedures to make voltage measurements through remote control on the KFM2150.

Measurement functions of the KFM2150

There are three types of measurement functions on the KFM2150: impedance measurement, voltage measurement, and current measurement. The impedance measurement function is classified in the sequence 1 group while the voltage and current measurement functions are classified in the sequence 2 group. These two sequences are completely independent in the measurement operations of the KFM2150.