Impedance measurement (current interrupt method)

IMP:CURR:PULS:TRAN

Sets the pulse transition time of the current interrupt method.

Command

[SENSe:]IMPedance:CURRent:PULSe:TRANsition[:LEADing] {<numeric>|MIN|MAX|DEF}

[SENSe:]IMPedance:CURRent:PULSe:TRANsition[:LEADing]? [{MIN|MAX}]

Parameter

Value: | 0.000 01 to 0.01 (0.01E-3 to 10E-3): (default 0.000 01)
Unit: | S (second)

Table 4 shows the setting that is specified when *RST, *RCL, or MEAS? is sent.

Response

Returns the pulse transition time of the current interrupt method in the NR3 form in response to IMP:CURR:PULS:TRAN?.

IMP:CURR:PULS:WIDT

Sets the pulse width of the current interrupt method.

Command

[SENSe:]IMPedance:CURRent:PULSe:WIDTh {<numeric>|MIN|MAX|DEF}

[SENSe:]IMPedance:CURRent:PULSe:WIDTh? [{MIN|MAX}]

Parameter

Value: | 0.000 1 to 0.01 (0.1E-3 to 10E-3): (default: 0.01)
Unit: | S (second)

Table 4 shows the setting that is specified when *RST, *RCL, or MEAS? is sent.

Response

Returns the pulse width of the current interrupt method in the NR3 form in response to IMP:CURR:PULS:WIDT?.

IMP:CURR:PULS:DEPT:RAT

Sets the pulse depth of the current interrupt method as a percentage.

Command

[SENSe:]IMPedance:CURRent:PULSe:DEPTh:RATio {<numeric>|MIN|MAX|DEF}

[SENSe:]IMPedance:CURRent:PULSe:DEPTh:RATio? [{MIN|MAX}]

Parameter

Value: | 0 to 100 (default: 100)
Unit: | PCT (%)

Table 4 shows the setting that is specified when *RST, *RCL, or MEAS? is sent.

Response

Returns the percentage of the pulse depth of the current interrupt method in the NR3 form in response to IMP:CURR:PULS:DEPT:RAT?.

IMP:CURR:PULS:DEPT

Sets the pulse depth of the current interrupt method as a current value.

Command

[SENSe:]IMPedance:CURRent:PULSe:DEPTh[:LEVel] {<numeric>|MIN|MAX|DEF}

[SENSe:]IMPedance:CURRent:PULSe:DEPTh[:LEVel]? [{MIN|MAX}]

Parameter

Value: | 0 to the rated load current of the PLZ-4W (The default setting is the present DC load current setting (SOUR:CURR))
Unit: | A

Table 4 shows the setting that is specified when *RST, *RCL, or MEAS? is sent.

Response

Returns the pulse depth of the current interrupt method in the NR3 form in response to IMP:CURR:PULS:DEPT?.

IMP:CURR:PULS:DEPT:RAT?.

IMP:SAMP:POS

Sets the sampling start position (Position: time from interrupt start) of the current interrupt method.

Command

[SENSe:]IMPedance:SAMPling:POSition {<numeric>|MIN|MAX|DEF}

[SENSe:]IMPedance:SAMPling:POSition? [{MIN|MAX]}

Parameter

Value: | 0 to 0.009 99 (0 to 9.99E-3): (default: 0.000 06)
Unit: | S (second)

Table 4 shows the setting that is specified when *RST, *RCL, or MEAS? is sent.

Response

Returns the sampling start position (Position: time from interrupt start) in the NR3 form in response to IMP:SAMP:POS?.

IMP:CURR:PULS:DEPT:RAT?.

IMP:SAMP:REG

Sets the sampling region of the current interrupt method.

Command

[SENSe:]IMPedance:SAMPling:REGion {<numeric>|MIN|MAX|DEF}

[SENSe:]IMPedance:SAMPling:REGion? [{MIN|MAX}]

Parameter

Value: | 0.000 002 to 0.000 51 (0.002E-3 to 0.51E-3): (default: 0.000 03)
Unit: | S (second)

Table 4 shows the setting that is specified when *RST, *RCL, or MEAS? is sent.

Response

Returns the sampling region of the current interrupt method in the NR3 form in response to IMP:SAMP:REG?.