This manual describes the procedure for connecting the interface and the procedure for transmitting commands to the KFM2150 using SCPI commands.

Overview

In addition to using the front panel, the KFM2150 can be controlled remotely using the following interfaces.

• GPIB interface

• RS232C interface

• USB interface

The interface type is selected from the panel.

The remote interface complies with IEEE Std 488.2-1991 and SCPI Specification 1999.0.

Use the SCPI commands only after you have understood the SCPI command syntax on the KFM2150.