Overview of Messages | Command Syntax
Parameters | Default settings

Default settings

Table 3 shows the default conditions when *RST, CONF:VOLT, CONF:VOLT:ALL, or MEAS? is sent and when the KFM2151 is shipped from the factory. When the power is turned on, the parameters in Table 3 are set to the settings that existed when the POWER switch was turned off.

Table 3 Default settings

Setup Item | Setting | Unit | Function
*RST Factory Default | CONF MEAS?*1
CHAN:VOLT:TERM | *2 | No change | - | Sets the channels on which to perform voltage scanning.
CHAN:VOLT:NSEL | 1 | - | Specify the channel on which to perform voltage scanning.
CHAN:ROUT:TERM | *3 | - | Sets the channels on which to perform impedance scanning.
CHAN:ROUT:NSEL | 1 | - | Specify the channel on which to perform impedance scanning.
VOLT:RANG | 200 | *4 | - | Sets the voltage range.
VOLT:RANG:AUTO | ON | - | Sets the voltage range to auto.
VOLT:PROT | 200 | 200 | V | Sets the voltage protection (OVP).
VOLT:PROT:LOW | -2.00 | -2.00 | V | Sets the voltage protection (UVP).

*1. When CONF:VOLT, CONF:VOLT:ALL, MEAS:VOLT?, or MEAS:ARR:VOLT? is sent.

*2. Chan: 1, termｱ: 01, voltage scanning: on

*3. Chan: 1, term±: 01, impedance scanning: on

*4. Range specified by CONF:VOLT, CONF:VOLT:ALL, and MEAS?