Soft start

INP:SST:RISE

Sets the soft start rising time and executes soft start (rising edge). If the command is set during the soft start rise time, the new value takes effect.

Command

INPut:SSTart:RISE {<numeric>|MIN|MAX|DEF}

Parameter

Value: | 0 to 7 200 (default: 0)
Unit: | S (second)

Table 4 shows the setting that is specified when *RST or *RCL is sent.

INP:SST:FALL

Sets the soft start falling time and executes soft start (falling edge). If the command is set during the soft start fall time, the new value takes effect.

Command

INPut:SSTart:FALL {<numeric>|MIN|MAX|DEF}

Parameter

Value: | 0 to 7 200 (default: 0)
Unit: | S (second)

Table 4 shows the setting that is specified when *RST or *RCL is sent.

INP:SST:RTIM

Queries the remaining time of soft start rising edge or soft start falling edge.

Command

INPut:SSTart:RTIMe?

Response

Returns the remaining time of soft start rising edge or falling edge in the NR1 form in response to INP:SST:RTIM?.

Unit: | S (second)