Function Search

IEEE488.2 common commands | Measurement Function Setup
Load On/Off and Input Terminal Setup | Electronic Load Setup | Waveform Data Setup
Measurement Operation and Trigger Function | System Configuration | Register

IEEE488.2 common commands
| *CLS | Clears the status data structures.
| *ESE | Sets the event status enable register bits.
| *ESR | Queries the event status register.
| *IDN | Queries the identification string (manufacturer information).
| *OPC | Causes the device to generate the operation complete message in the event status register when all pending selected device operations have been finished.
| *RCL | Recalls the contents saved to the memory.
| *RST | Performs a device reset. Configures the KFM2150 to a known condition independent from the usage history of the device.
| *SAV | Saves the current settings to the memory.
| *SRE | Sets the service request enable register bits.
| *STB | Reads the status byte and master summary status bits.
| *TRG | Trigger command
| *TST | Since there is no self-test function built into the KFM2150.
| *WAI | Prevents the device from executing subsequent commands or queries until the No Operation Pending flag becomes true.

>>TOP

Measurement Function Setup
Impedance measurement (AC impedance method)
| IMP:CURR:AC | Averaging period of the measured value
| IMP:CURR:AC:RAT | Measuring AC current (percentage)
| IMP:CURR:AC FREQ | Measuring frequency
Impedance measurement (current interrupt method)
| IMP:CURR:PULS:TRAN | Pulse transition time
| IMP:CURR:PULS:WIDT | Pulse width
| IMP:CURR:PULS:DEPT:RAT | Pulse depth
| IMP:CURR:PULS:DEPT | Pulse depth (current)
| IMP:SAMP:POS | Sampling start position
| IMP:SAMP:REG | Sampling region
Impedance measurement (averaging)
| IMP:AVER:MOV:COUN | Moving average count
| IMP:AVER:MOV:CLE | Moving average area
Measurement method
| METH | Measurement method
Voltage measurement
| VOLT:PROT:LOW | Voltage sensing undervoltage protection
| VOLT:PROT:LOW:DEL | Voltage sensing undervoltage protection delay time

>>TOP

Load On/Off and Input Terminal Setup
Load on/off
| INP | Load on/off
| INP:PROT:CLE | Alarm clear
Soft start
| INP:SST:RISE | Soft start falling edge
| INP:SST:FALL | Soft start rising edge
| INP:SST:RTIM | Remaining time
VOLTAGE SENSING terminal
| INP:SENS:VOLT | VOLTAGE SENSING channel
CURRENT SENSING terminal
| INP:SENS:CURR | CURRENT SENSING channel

>>TOP

Electronic Load Setup
| SOUR:CURR | AC current limit
| SOUR:CURR:EXT | External electronic load DC current
| SOUR:CURR:RANG | Electronic load DC current range
| SOUR:VOLT | Voltage of PLZ-4W Series
| SOUR:VOLT:RANG | Voltage range of PLZ-4W Series
| SOUR:VOLT:PROT:LOW | Undervoltage protection
| SOUR:POW:PROT | PLZ-4W OPP activation voltage of the electronic load DC voltage

>>TOP

Waveform Data Setup
| FORM:BORD | Data transmission/recording mode
| FORM:PAGE:STAR | Length of the data to be transferred
| FORM:PAGE:LENG | Start point of the data to be transferred
| TRAC | Voltage waveform data or current waveform data

>>TOP

Measurement Operation and Trigger Function
Trigger function
| TRIG:COUN | Sequence 1: Trigger count
| TRIG:SEQ2:COUN | Sequence 2: Trigger count
| TRIG:TIM | Sequence 1: Trigger time setting
| TRIG:SEQ2:TIM | Sequence 2: Trigger time setting
| TRIG:SOUR | Sequence 1: Trigger source
| TRIG:SEQ2:SOUR | Sequence 2: Trigger source
| INIT | Sequence 1 and 2: Start the trigger function
| INIT:SEQ | Sequence 1: Start the trigger function
| INIT:SEQ2 | Sequence 2: Start the trigger function
| INIT:SEQ:WAV | Sequence 1: Starts the trigger function while holding the voltage and current waveform data
| ABOR | Aborts the sequence 1 and 2 operations
| *TRG or IEEE488.1 get (Group Execute Trigger) | Software trigger
| *RCL / *RST | Recall or Reset
Measurement operation
| FETC / FETC:ARR | Queries the measured data
| READ / READ:ARR | Starts the measurement and queries the data
| MEAS:<meter_fn> / MEAS:ARR:<meter_fn> | Resets a portion of the settings to default, start the measurement, and queries the data

>>TOP

System Configuration
| SYST:COMM:SER:PACE | Flow control condition
| SYST:ERR | Reads the error information
| SYST:LOC (RS232C and USB only) | Sets to local
| SYST:REM (RS232C and USB only) | Sets the KFM2150 control to remote. Locks panels keys except the local key
| SYST:RWL (RS232C and USB only) | Sets the KFM2150 control to remote. Locks the panel operation.
| SYST:VERS | Version of the SCPI specifications to which the KFM2150 conforms

>>TOP

Register
Status byte register
Event status register
OPERation status register
| STAT:OPER | Queries the event
| STAT:OPER:COND | Queries the condition of the register
| STAT:OPER:ENAB | Enable register
| STAT:OPER:NTR | Negative transition
| STAT:OPER:PTR | Positive transition
OPERation:MEASuring status register
| STAT:OPER:MEAS | Queries the event
| STAT:OPER:MEAS:COND | Queries the condition of the register
| STAT:OPER:MEAS:ENAB | Enable register
| STAT:OPER:MEAS:NTR | Negative transition
| STAT:OPER:MEAS:PTR | Positive transition
OPERation:TRIGger status register
| STAT:OPER:TRIG | Queries the event
| STAT:OPER:TRIG:COND | Queries the condition of the register
| STAT:OPER:TRIG:ENAB | Enable register
| STAT:OPER:TRIG:NTR | Negative transition
| STAT:OPER:TRIG:PTR | Positive transition
OPERation:PROTecting status register
| STAT:OPER:PROT | Queries the event
| STAT:OPER:PROT:COND | Queries the condition of the register
| STAT:OPER:PROT:ENAB | Enable register
| STAT:OPER:PROT:NTR | Negative transition
| STAT:OPER:PROT:PTR | Positive transition
QUEStionable status register
| STAT:QUES | Queries the event
| STAT:QUES:COND | Queries the condition of the register
| STAT:QUES:ENAB | Enable register
| STAT:QUES:NTR | Negative transition
| STAT:QUES:PTR | Positive transition
Preset Status
| STAT:PRES | Constructing status data

>>TOP