System Configuration

Configures the KFM2150 system.

SYST:ERR

Reads the oldest error information from the error queue. The error queue can store up to 255 errors.

Command

SYSTem:ERRor[:NEXT]?

Response

Returns the oldest error in the error queue in response to SYST:ERR? as follows:

(Example) When there are no errors or events
Returns 0, "No error".

(Example) When a command that cannot be executed in the current operating condition is received
Returns -221, "Settings conflict".

SYST:LOC (RS232C and USB only)

Sets the KFM2150 operation to panel operation (local). This is a substitute command for the IEEE488.1 gtl message (Go To Local).

Command

SYSTem:LOCal

SYST:REM (RS232C and USB only)

Sets the KFM2150 operation to remote mode. All panel keys except the LOCAL key are locked. This is a substitute command for the IEEE488.1 REN message (Remote Enable) and address designation.

Omitting the parameter is equivalent to ON (1).

The power-on default is ON for the RS232C and OFF for the USB.

Command

SYSTem:REMote

SYST:RWL (RS232C and USB only)

Sets the KFM2150 operation to remote mode. All panel keys are locked (LOCAL key is also locked). This is a substitute command for the IEEE488.1 llo message (Local Lock Out).

Command

SYSTem:RWLock

SYST:VERS

Queries the version of the SCPI specifications to which the KFM2150 conforms.

Command

SYSTem:VERSion?

Response

Returns SCPI 1999.0 in response to SYST:VERS?.

SYST:COMM:SER:PACE (RS232C only)

Sets the flow control condition of the KFM2150 serial (RS232C) interface.

Command

SYSTem:COMMunicate:SERial:PACE {XON|ACK}

SYSTem:COMMunicate:SERial:PACE?

Parameter

Value: | XON | X-Flow control
| ACK | Control using the acknowledge function

Response

Returns the flow control condition in response to SYST:COMM:SER:PACE?.