Impedance measurement (averaging)

IMP:AVER:MOV:COUN

Sets the moving average count.

Command

[SENSe:]IMPedance:AVERage:MOVing:COUNt{<numeric>|MIN|MAX|DEF}

[SENSe:]IMPedance:AVERage:MOVing:COUNt? [{MIN|MAX}]

Parameter

Value: | 1 to 256 (default: 1)
Resolution: | 1

Table 4 shows the setting that is specified when *RST, *RCL, or MEAS? is sent.

Response

Returns the moving average count in the NR1 form in response to IMP:AVER:MOV:COUN?.

IMP:AVER:MOV:CLE

Clears the moving average.

Command

[SENSe:]IMPedance:AVERage:MOVing:CLEar