QUEStionable status register

The QUEStionable status register is a 16-bit register that stores information related to the questionable events and status during KFM2150 operation.

These register bits may indicate problems with the measured data of the KFM2150.

Table 12 QUEStionable status register (STATus:QUEStionable)

Bit | Bit Weight | Bit Name | Description
0 | 1 | VOLTage | The voltage measurement data is questionable.
1 | 2 | CURRent | The current measurement data is questionable.
2 | 4 | Not Used | Not Used
3 | 8 | Not Used | Not Used
4 | 16 | Not Used | Not Used
5 | 32 | Not Used | Not used
6 | 64 | Not Used | Not used
7 | 128 | Not Used | Not Used
8 | 256 | Not Used | Not Used
9 | 512 | IMPedance | Impedance measurement data is questionable.
10 | 1024 | PLZ4w COMMunication | PLZ4W communication is questionable.
11 | 2048 | Not Used | Not Used
12 | 4096 | Not Used | Not Used
13 | 8192 | Not Used | Not used
14 | 16384 | Not Used | Not used
15 | 32768 | Not Used | Always zero

STAT:QUES

Queries the event of the QUEStionable status register.

A query clears the contents of the register.

Command

STATus:QUEStionable[:EVENt]?

Response

Returns the event of the QUEStionable status register in the NR1 form.

STAT:QUES:COND

Queries the condition of the QUEStionable status register.

A query does not clear the contents of the register.

Command

STATus:QUEStionable:CONDition?

Response

Returns the condition of the QUEStionable status register in the NR1 form.

STAT:QUES:ENAB

Sets the enable register of the QUEStionable status register.

Command

STATus:QUEStionable:ENABle <NR1>

STATus:QUEStionable:ENABle?

Parameter

Value: 0 to 32767

Response

Returns the enable register setting of the QUEStionable status register in the NR1 form.

STAT:QUES:PTR

Sets the positive transition of the QUEStionable status register.

Command

STATus:QUEStionable:PTRansition <NR1>

STATus:QUEStionable:PTRansition?

Parameter

Value: 0 to 32767

Response

Returns the positive transition of the QUEStionable status register in the NR1 form.

STAT:QUES:NTR

Sets the negative transition of the QUEStionable status register.

Command

STATus:QUEStionable:NTRansition <NR1>

STATus:QUEStionable:NTRansition?

Parameter

Value: 0 to 32767

Response

Returns the negative transition of the QUEStionable status register in the NR1 form.