<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >
<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >
<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>DVD-RV20/DVD-RV10</Model>
<System>ORDER NO.ODSD000401C1</System>
<SubSystem>DVD Player</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0200000000x</ModuleTitle>
<IssueNo issue=1>
<IssueDate day=25 month=Jul year=2000>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>DVD-RV20/DVD-RV10</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>
<Body>
<Descriptive>
<Title>2 PREVENTION OF ELECTRO STATIC DISCHARGE (ESD) TO ELECTROSTATICALLY SENSITIVE (ES) DEVICES</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
rv20u
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0101020000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0300000000x
</nmlist>
</nameloc>
</Para>
<Para>Some semiconductor (solid state) devices can be damaged easily by static electricity.  Such components commonly are called Electrostatically Sensitive (ES) Devices. Examples of typical ES devices are integrated circuits and some field-effect transistorsand semiconductor  "chip" components.  The following techniques should be used to help reduce the incidence of component damage caused by electro static discharge (ESD).</Para>
<Para><seqlist><item><Para>Immediately before handling any semiconductor component or semiconductor-equipped assembly, drain off any ESD on your body by touching a known earth ground.  Alternatively, obtain and wear a commercially available dischargingESD wrist strap, which should be removed for potential shock reasons prior to applying power to the unit under test.</Para>
</item>
<item><Para>After removing an electrical assembly equipped with ES devices, place the assembly on a conductive surface such as alminum foil, to prevent electrostatic charge buildup or exposure of the assembly.</Para>
</item>
<item><Para>Use only a grounded-tip soldering iron to solder or unsolder ES devices.</Para>
</item>
<item><Para>Use only an anti-static solder removal device.  Some solder removal devices not classified as "anti-static (ESD protected)" can generate electrical charge sufficient to damage ES devices.</Para>
</item>
<item><Para>Do not use freon-propelled chemicals.   These can generate electrical charges sufficient to damage ES devices.</Para>
</item>
<item><Para>Do not remove a replacement ES device from its protective package until immediately before you are ready to install it. (Most replacement ES devices are packaged with leads electrically shorted together by conductive foam, alminum foil or comparableconductive material).</Para>
</item>
<item><Para>Immediately before removing the protective material from the leads of a replacement ES device, touch the protective material to the chassis or circuit assembly into which the device will be installed.</Para>
<Para><emphasis>Caution</emphasis></Para>
<Para>Be sure no power is applied to the chassis or circuit, and observe all other safety precautions.</Para>
</item>
<item><Para>Minimize bodily motions when handling unpackaged replacement ES devices. (Otherwise hamless motion such as the brushing together of your clothes fabric or the lifting of your foot from a carpeted floor can generate static electricity (ESD) sufficient todamage an ES device).</Para>
</item>
</seqlist>
</Para>
<Figure><graphic boardno="graphic5" reprowid="163.746MM" reprodep="28.534MM" location="internal"></Figure>
<!-- Footer -->
<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
rv20u
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0101020000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0300000000x
</nmlist>
</nameloc>
</Para>
</Descriptive>
&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
