<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >
<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >
<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>DVD-RV20/DVD-RV10</Model>
<System>ORDER NO.ODSD000401C1</System>
<SubSystem>DVD Player</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0101010000</ModuleTitle>
<IssueNo issue=1>
<IssueDate day=25 month=Jul year=2000>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>DVD-RV20/DVD-RV10</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>
<Body>
<Descriptive>
<Title>1.1.1 LEAKAGE CURRENT COLD CHECK</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
rv20u
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0101000000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0101020000
</nmlist>
</nameloc>
</Para>
<Para><seqlist><item><Para>Unplug the AC cord and connect a jumper between the two prongs on the plug.</Para>
</item>
<item><Para>Measure the resistance value, with an ohmmeter, between the jumpered AC plug and each exposed metallic cabinet part on the equipment such as screwheads, connectors, control shafts, etc.  When the exposed metallic part has a return path to thechassis, the reading should be between 1M&ohm; and 5.2M&ohm;./ When the exposed metal does not have a return path to the chassis, the reading must be<graphic boardno="graphic3" reprowid="3.000MM" reprodep="2.117MM" location="internal">.</Para>
<Figure><graphic boardno="graphic4" reprowid="88.000MM" reprodep="45.551MM" location="internal"></Figure>
</item>
</seqlist>
</Para>
<!-- Footer -->
<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
rv20u
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0101000000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0101020000
</nmlist>
</nameloc>
</Para>
</Descriptive>
&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
