<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >
<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >
<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>DVD-RV20/DVD-RV10</Model>
<System>ORDER NO.ODSD000401C1</System>
<SubSystem>DVD Player</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s1202000000</ModuleTitle>
<IssueNo issue=1>
<IssueDate day=25 month=Jul year=2000>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>DVD-RV20/DVD-RV10</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>
<Body>
<Descriptive>
<Title>12.2 Video Output (Chrominance Signal) Adjustment</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
rv20u
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s1201000000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s1300000000x
</nmlist>
</nameloc>
</Para>
<Para>Do this adjustment after replacing a C.B.A.</Para>
<Table frame="ALL" colsep="1" rowsep="1"><tgroup cols="4" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="1.476in"><colspec colnum="2" colname="2" colwidth="1.476in"><colspec colnum="3" colname="3" colwidth="1.476in"><colspec colnum="4" colname="4" colwidth="1.476in"><thead><row rowsep="1"><entry colname="1" align="CENTER"><Para>Measurement point</Para>
</entry>
<entry colname="2" align="CENTER"><Para>Adjustment point</Para>
</entry>
<entry colname="3" align="CENTER"><Para>Mode</Para>
</entry>
<entry colname="4" align="CENTER"><Para>Disc</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="CENTER"><Para>Video output terminal</Para>
</entry>
<entry colname="2" align="CENTER"><Para>VR3511 (mother C.B.A.)</Para>
</entry>
<entry colname="3" align="CENTER"><Para>Color bar 75&percnt;</Para>
<Para>PLAY (Title 46):DVDT-S15</Para>
<Para>PLAY (Title 12):DVDT-S01</Para>
</entry>
<entry colname="4" align="CENTER"><Para>DVDT-S15</Para>
<Para>or</Para>
<Para>DVDT-S01</Para>
</entry>
</row>
<row rowsep="1"><entry namest="1" nameend="2" align="CENTER"><Para>Measuring equipment, tools</Para>
</entry>
<entry namest="3" nameend="4" align="CENTER"><Para>Adjustment value</Para>
</entry>
</row>
<row rowsep="0"><entry namest="1" nameend="2" align="CENTER"><Para>Screwdriver,Oscilloscope</Para>
<Para>200mV&sol;div, 10&micro;sec&sol;div</Para>
</entry>
<entry namest="3" nameend="4" align="CENTER"><Para>621mVp-p&plusmn;12mV</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<Para>Purpose: To maintain video signal output compatibility.</Para>
<Para><seqlist><item><Para>Connect the oscilloscope to the video output terminal and terminate at 75 ohms.</Para>
</item>
<item><Para>Adjust VR3511 so that the chrominance signal (C) level becomes 621 mVp-p&plusmn;12 mV.</Para>
<Figure><graphic boardno="graphic64" reprowid="183.000MM" reprodep="57.658MM" location="internal"></Figure>
</item>
</seqlist>
</Para>
<!-- Footer -->
<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
rv20u
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s1201000000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s1300000000x
</nmlist>
</nameloc>
</Para>
</Descriptive>
&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
