<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >
<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >
<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>DVD-RV20/DVD-RV10</Model>
<System>ORDER NO.ODSD000401C1</System>
<SubSystem>DVD Player</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0601000000</ModuleTitle>
<IssueNo issue=1>
<IssueDate day=25 month=Jul year=2000>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>DVD-RV20/DVD-RV10</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>
<Body>
<Descriptive>
<Title>6.1 Service Mode Table</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
rv20u
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0600000000x
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0602000000
</nmlist>
</nameloc>
</Para>
<Para>The service modes can be activated by pressing various button combinations on the player and remote control unit.</Para>
<Table frame="ALL" colsep="1" rowsep="1"><tgroup cols="4" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.984in"><colspec colnum="2" colname="2" colwidth="1.772in"><colspec colnum="3" colname="3" colwidth="2.953in"><colspec colnum="4" colname="4" colwidth="1.378in"><thead><row rowsep="1"><entry colname="1" align="CENTER"><Para>Player buttons</Para>
</entry>
<entry colname="2" align="CENTER"><Para>Remote control unit buttons</Para>
</entry>
<entry colname="3" align="CENTER"><Para>Application</Para>
</entry>
<entry colname="4" align="CENTER"><Para>Note</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" morerows="6" align="CENTER"><Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para>PAUSE</Para>
<Para>&plus;</Para>
<Para>OPEN&sol;CLOSE</Para>
</entry>
<entry colname="2" align="CENTER"><Para>0</Para>
</entry>
<entry colname="3" align="LEFT"><Para>Displaying the UHF display F_ _ _</Para>
</entry>
<entry colname="4" align="LEFT"><Para>Refer to section 6.2, Self-</Para>
<Para>Diagnosis Function (UHF</Para>
<Para>Display).</Para>
</entry>
</row>
<row rowsep="1"><entry colname="2" align="CENTER"><Para>5</Para>
</entry>
<entry colname="3" align="LEFT"><Para>Jitter check, Tilt adjustment</Para>
<Para>&ast;Display shows JITXXX</Para>
<Para>The 3 digit number (JITXXX) indicates the Jitter rate (JIT088&equals;8.8&percnt;)</Para>
<Para>The3 digit number the right of JITXXX displays an error counter (increases as errors occur) but does not necessarily mean picture&sol; playback problems will occur.</Para>
<Para>(This numberis not as important as the JITXXX) Refer to section 11.14 for Optical Pickup Tilt Adjustment Procedure</Para>
</entry>
<entry colname="4" align="LEFT"><Para>Refer to section 11.14,</Para>
<Para>Optical Pickup Tilt</Para>
<Para>Adjustment.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="2" align="CENTER"><Para>6</Para>
</entry>
<entry colname="3" align="LEFT"><Para>Checking the region numbers and broadcast system</Para>
</entry>
<entry colname="4" align="LEFT"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="2" align="CENTER"><Para>7</Para>
</entry>
<entry colname="3" align="LEFT"><Para>Checking the program version</Para>
</entry>
<entry colname="4" align="LEFT"><Para>Check the IC6302</Para>
<Para>FLASH ROM program.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="2" align="CENTER"><Para>9</Para>
</entry>
<entry colname="3" align="LEFT"><Para>Lighting Confirmation Function of Display Tube</Para>
</entry>
<entry colname="4" align="LEFT"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="2" align="CENTER"><Para>DISPLAY</Para>
</entry>
<entry colname="3" align="LEFT"><Para>Checking the laser drive current</Para>
</entry>
<entry colname="4" align="LEFT"><Para>Refer to section 5,</Para>
<Para>Optical Pickup</Para>
<Para>Self-Diagnosis and</Para>
<Para>Replacement</Para>
</entry>
</row>
<row rowsep="1"><entry colname="2" align="CENTER"><Para>PAUSE</Para>
</entry>
<entry colname="3" align="LEFT"><Para>Writing the laser drive current value after replacing</Para>
<Para>the optical pickup (do not use for anything other than</Para>
<Para>optical pickup replacement)</Para>
</entry>
<entry colname="4" align="LEFT"><Para>Procedure.</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="LEFT"><Para>PAUSE</Para>
<Para>SKIP&sol;SEARCH&lt;&lt;</Para>
<Para>OPEN&sol;CLOSE</Para>
</entry>
<entry colname="2" align="CENTER"><Para></Para>
</entry>
<entry colname="3" align="LEFT"><Para>Initializing the DVD player</Para>
<Para>(restoring factory preset settings)/&ast;Use when replaceing a microprocessor, microprocessor peripheral parts, or C.B.A.</Para>
</entry>
<entry colname="4" align="LEFT"><Para>Refer to section 10.1, Initializing the DVD</Para>
<Para>Player</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<!-- Footer -->
<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
rv20u
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0600000000x
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0602000000
</nmlist>
</nameloc>
</Para>
</Descriptive>
&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
