<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >
<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >
<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>DVD-RV20/DVD-RV10</Model>
<System>ORDER NO.ODSD000401C1</System>
<SubSystem>DVD Player</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s1300000000x</ModuleTitle>
<IssueNo issue=1>
<IssueDate day=25 month=Jul year=2000>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>DVD-RV20/DVD-RV10</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>
<Body>
<Descriptive>
<Title>13 Abbreviations</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
rv20u
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s1202000000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s1400000000x
</nmlist>
</nameloc>
</Para>
<Table frame="ALL" colsep="1" rowsep="1"><tgroup cols="3" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.394in"><colspec colnum="2" colname="2" colwidth="0.787in"><colspec colnum="3" colname="3" colwidth="2.165in"><thead><row rowsep="1"><entry namest="1" nameend="2" align="CENTER"><Para>INITIAL&sol;LOGO</Para>
</entry>
<entry colname="3" align="CENTER"><Para>ABBREVIATIONS</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="CENTER"><Para>A</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>A0~UP</Para>
<Para>ACLK</Para>
<Para>AD0~UP</Para>
<Para>ADATA</Para>
<Para>ALE</Para>
<Para>AMUTE</Para>
<Para>AREQ</Para>
<Para>ARF</Para>
<Para>ASI</Para>
<Para>ASO</Para>
<Para>ASYNC</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>ADDRESS</Para>
<Para>AUDIO CLOCK</Para>
<Para>ADDRESS BUS</Para>
<Para>AUDIO PES PACKET DATA</Para>
<Para>ADDRESS LATCH ENABLE</Para>
<Para>AUDIO MUTE</Para>
<Para>AUDIO PES PACKET REQUEST</Para>
<Para>AUDIO RF</Para>
<Para>SERVO AMP INVERTED INPUT</Para>
<Para>SERVO AMPOUTPUT</Para>
<Para>AUDIO WORD DISTINCTION SYNC</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="CENTER"><Para>B</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>BCK</Para>
<Para>BCKIN</Para>
<Para>BDO</Para>
<Para>BLKCK</Para>
<Para>BOTTOM</Para>
<Para>BYP</Para>
<Para>BYTCK</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>BIT CLOCK (PCM)</Para>
<Para>BIT CLOCK INPUT</Para>
<Para>BLACK DROP OUT</Para>
<Para>SUB CODE BLOCK CLOCK</Para>
<Para>CAP. FOR BOTTOM HOLD</Para>
<Para>BYPATH</Para>
<Para>BYTE CLOCK</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="CENTER"><Para>C</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>CAV</Para>
<Para>CBDO</Para>
<Para>CD</Para>
<Para>CDSCK</Para>
<Para>CDSRDATA</Para>
<Para>CDRF</Para>
<Para>CDV</Para>
<Para>CHNDATA</Para>
<Para>CKSL</Para>
<Para>CLV</Para>
<Para>COFTR</Para>
<Para>CPA</Para>
<Para>CPCS</Para>
<Para>CPDT</Para>
<Para>CPUADR</Para>
<Para>CPUADT</Para>
<Para>CPUIRQ</Para>
<Para>CPRD</Para>
<Para>CPWR</Para>
<Para>CS</Para>
<Para>CSYNCIN</Para>
<Para>CSYNCOUT</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>CONSTANT ANGULAR VELOCITY</Para>
<Para>CAP. BLACK DROP OUT</Para>
<Para>COMPACT DISC</Para>
<Para>CD SERIAL DATA CLOCK</Para>
<Para>CD SERIAL DATA</Para>
<Para>CD RF (EFM) SIGNAL</Para>
<Para>COMPACT DISC-VIDEO</Para>
<Para>CHANNEL DATA</Para>
<Para>SYSTEM CLOCKSELECT</Para>
<Para>CONSTANT LINEAR VELOCITY</Para>
<Para>CAP. OFF TRACK</Para>
<Para>CPU ADDRESS</Para>
<Para>CPU CHIP SELECT</Para>
<Para>CPU DATA</Para>
<Para>CPU ADDRESS LATCH</Para>
<Para>CPU ADDRESS DATA BUS</Para>
<Para>CPU INTERRUPT REQUEST</Para>
<Para>CPU READ ENABLE</Para>
<Para>CPU WRITE ENABLE</Para>
<Para>CHIPSELECT</Para>
<Para>COMPOSITE SYNC IN</Para>
<Para>COMPOSITE SYNC OUT</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="CENTER"><Para>D</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>DACCK</Para>
<Para>DEEMP</Para>
<Para>DEMPH</Para>
<Para>DIG0~UP</Para>
<Para>DIN</Para>
<Para>DMSRCK</Para>
<Para>DMUTE</Para>
<Para>DO</Para>
<Para>DOUT0~UP</Para>
<Para>DRF</Para>
<Para>DRPOUT</Para>
<Para>DREQ</Para>
<Para>DRESP</Para>
<Para>DSC</Para>
<Para>DSLF</Para>
<Para>DVD</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>D&sol;A CONVERTER CLOCK</Para>
<Para>DEEMPHASIS BIT ON&sol;OFF</Para>
<Para>DEEMPHASIS SWITCHING</Para>
<Para>FL DIGIT OUTPUT</Para>
<Para>DATA INPUT</Para>
<Para>DM SERIAL DATA READ CLOCK</Para>
<Para>DIGITAL MUTE CONTROL</Para>
<Para>DROP OUT</Para>
<Para>DATAOUTPUT</Para>
<Para>DATA SLICE RF (BIAS)</Para>
<Para>DROP OUT SIGNAL</Para>
<Para>DATA REQUEST</Para>
<Para>DATA RESPONSE</Para>
<Para>DIGITAL SERVO CONTROLLER</Para>
<Para>DATA SLICE LOOP FILTER</Para>
<Para>DIGITAL VIDEO DISC</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<Table frame="ALL" colsep="1" rowsep="1"><tgroup cols="3" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.394in"><colspec colnum="2" colname="2" colwidth="0.787in"><colspec colnum="3" colname="3" colwidth="2.165in"><thead><row rowsep="1"><entry namest="1" nameend="2" align="CENTER"><Para>INITIAL&sol;LOGO</Para>
</entry>
<entry colname="3" align="CENTER"><Para>ABBREVIATIONS</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="CENTER"><Para>E</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>EC</Para>
<Para>ECR</Para>
<Para></Para>
<Para>ENCSEL</Para>
<Para>ETMCLK</Para>
<Para>ETSCLK</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>ERROR TORQUE CONTROL</Para>
<Para>ERROR TORQUE CONTROL REFERENCE</Para>
<Para>ENCODER SELECT</Para>
<Para>EXTERNAL M CLOCK (81MHz&sol;40.5MHz)</Para>
<Para> EXTERNAL S CLOCK (54MHz)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="CENTER"><Para>F</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>FBAL</Para>
<Para>FCLK</Para>
<Para>FE</Para>
<Para>FFI</Para>
<Para>FEO</Para>
<Para>FG</Para>
<Para>FSC</Para>
<Para>FSCK</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>FOCUS BALANCE</Para>
<Para>FRAME CLOCK</Para>
<Para>FOCUS ERROR</Para>
<Para>FOCUS ERROR AMP INVERTED INPUT</Para>
<Para>FOCUS ERROR AMP OUTPUT</Para>
<Para>FREQUENCY GENERATOR</Para>
<Para>FREQUENCY SUB CARRIER</Para>
<Para>FS (384 OVER SAMPLING) CLOCK</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="CENTER"><Para>G</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>GND</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>COMMON GROUNDING (EARTH)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="CENTER"><Para>H</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>HA0~UP</Para>
<Para>HD0~UP</Para>
<Para>HINT</Para>
<Para>HRXW</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>HOST ADDRESS</Para>
<Para>HOST DATA</Para>
<Para>HOST INTERRUPT</Para>
<Para>HOST READ&sol;WRITE</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="CENTER"><Para>I</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>IECOUT</Para>
<Para>IPFRAG</Para>
<Para>IREF</Para>
<Para>ISEL</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>IEC958 FORMAT DATA OUTPUT</Para>
<Para>INTERPOLATION FLAG</Para>
<Para>I (CURRENT) REFERENCE</Para>
<Para>INTERFACE MODE SELECT</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="CENTER"><Para>L</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>LDON</Para>
<Para>LPC</Para>
<Para>LRCK</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>LASER DIODE CONTROL</Para>
<Para>LASER POWER CONTROL</Para>
<Para>L CH&sol;R CH DISTINCTION CLOCK</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="CENTER"><Para>M</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>MA0~UP</Para>
<Para>MCK</Para>
<Para>MCKI</Para>
<Para>MCLK</Para>
<Para>MDATA</Para>
<Para>MDQ0~UP</Para>
<Para>MDQM</Para>
<Para>MLD</Para>
<Para>MPEG</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>MEMORY ADDRESS</Para>
<Para>MEMORY CLOCK</Para>
<Para>MEMORY CLOCK INPUT</Para>
<Para>MEMORY SERIAL COMMAND CLOCK</Para>
<Para>MEMORY SERIAL COMMAND DATA</Para>
<Para>MEMORY DATA INPUT&sol;OUTPUT</Para>
<Para>MEMORY DATA I&sol;O MASK</Para>
<Para>MEMORYSERIAL COMMAND LOAD</Para>
<Para>MOVING PICTURE EXPERTS GROUP</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="CENTER"><Para>O</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>ODC</Para>
<Para>OFTR</Para>
<Para>OSCI</Para>
<Para>OSCO</Para>
<Para>OSD</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>OPTICAL DISC CONTROLLER</Para>
<Para>OFF TRACKING</Para>
<Para>OSCILLATOR INPUT</Para>
<Para>OSCILLATOR OUTPUT</Para>
<Para>ON SCREEN DISPLAY</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="CENTER"><Para>P</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>P1~UP</Para>
<Para>PCD</Para>
<Para>PCK</Para>
<Para>PDVD</Para>
<Para>PEAK</Para>
<Para>PLLCLK/PLLOK</Para>
<Para>PWMCTL</Para>
<Para>PWMDA</Para>
<Para>PWMOA, B</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>PORT</Para>
<Para>CD TRACKING PHASE DIFFERENCE</Para>
<Para>PLL CLOCK</Para>
<Para>DVD TRACKING PHASE DIFFERENCE</Para>
<Para>CAP. FOR PEAK HOLD</Para>
<Para>CHANNEL PLL CLOCK</Para>
<Para>PLL LOCK</Para>
<Para>PWM OUTPUT CONTROL</Para>
<Para>PULSE WAVE MOTOR DRIVEA</Para>
<Para>PULSE WAVE MOTOR OUT A, B</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<Table frame="ALL" colsep="1" rowsep="1"><tgroup cols="3" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.394in"><colspec colnum="2" colname="2" colwidth="0.787in"><colspec colnum="3" colname="3" colwidth="2.165in"><thead><row rowsep="1"><entry namest="1" nameend="2" align="CENTER"><Para>INITIAL&sol;LOGO</Para>
</entry>
<entry colname="3" align="CENTER"><Para>ABBREVIATIONS</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="CENTER"><Para>R</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>RE</Para>
<Para>RFENV</Para>
<Para>RFO</Para>
<Para>RS</Para>
<Para>RSEL</Para>
<Para>RST</Para>
<Para>RSV</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>READ ENABLE</Para>
<Para>RF ENVELOPE</Para>
<Para>RF PHASE DIFFERENCE OUTPUT</Para>
<Para>(CD-ROM) REGISTER SELECT</Para>
<Para>RF POLARITY SELECT</Para>
<Para>RESET</Para>
<Para>RESERVE</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="CENTER"><Para>S</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>SBI0, 1</Para>
<Para>SBO0</Para>
<Para>SBT0, 1</Para>
<Para>SCK</Para>
<Para>SCKR</Para>
<Para>SCL</Para>
<Para>SCLK</Para>
<Para>SDA</Para>
<Para>SEG0~UP</Para>
<Para>SELCLK</Para>
<Para>SEN</Para>
<Para>SIN1, 2</Para>
<Para>SOUT1, 2</Para>
<Para>SPDI</Para>
<Para>SPDO</Para>
<Para>SPEN</Para>
<Para>SPRCLK</Para>
<Para>SPWCLK</Para>
<Para>SQCK</Para>
<Para>SQCX</Para>
<Para>SRDATA</Para>
<Para>SRMADR</Para>
<Para>SRMDT0~7</Para>
<Para>SS</Para>
<Para>STAT</Para>
<Para>STCLK</Para>
<Para>STD0~UP</Para>
<Para>STENABLE</Para>
<Para>STSEL</Para>
<Para>STVALID</Para>
<Para>SUBC</Para>
<Para>SBCK</Para>
<Para>SUBQ</Para>
<Para>SYSCLK</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>SERIAL DATA INPUT</Para>
<Para>SERIAL DATA OUTPUT</Para>
<Para>SERIAL CLOCK</Para>
<Para>SERIAL DATA CLOCK</Para>
<Para>AUDIO SERIAL CLOCK RECEIVER</Para>
<Para>SERIAL CLOCK</Para>
<Para>SERIAL CLOCK</Para>
<Para>SERIAL DATA</Para>
<Para>FL SEGMENT OUTPUT</Para>
<Para>SELECTCLOCK</Para>
<Para>SERIAL PORT ENABLE</Para>
<Para>SERIAL DATA IN</Para>
<Para>SERIAL DATA OUT</Para>
<Para>SERIAL PORT DATA INPUT</Para>
<Para>SERIAL PORT DATA OUTPUT</Para>
<Para>SERIAL PORT R&sol;W ENABLE</Para>
<Para>SERIAL PORT READ CLOCK</Para>
<Para>SERIAL PORT WRITE CLOCK</Para>
<Para>SUB CODE Q CLOCK</Para>
<Para>SUBCODE Q DATA READ CLOCK</Para>
<Para>SERIAL DATA</Para>
<Para>SRAM ADDRESS BUS</Para>
<Para>SRAM DATA BUS 0~7</Para>
<Para>START&sol;STOP</Para>
<Para>STATUS</Para>
<Para>STREAM DATA CLOCK</Para>
<Para>STREAM DATA</Para>
<Para>STREAM DATA INPUT ENABLE</Para>
<Para>STREAM DATA POLARITY SELECT</Para>
<Para>STREAM DATAVALIDITY</Para>
<Para>SUB CODE SERIAL</Para>
<Para>SUB CODE CLOCK</Para>
<Para>SUB CODE Q DATA</Para>
<Para>SYSTEM CLOCK</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="CENTER"><Para>T</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>TE</Para>
<Para>TIBAL</Para>
<Para>TID</Para>
<Para>TIN</Para>
<Para>TIP</Para>
<Para>TIS</Para>
<Para>TPSN</Para>
<Para>TPSO</Para>
<Para>TPSP</Para>
<Para>TRCRS</Para>
<Para>TRON</Para>
<Para>TRSON</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>TRACKING ERROR</Para>
<Para>BALANCE CONTROL</Para>
<Para>BALANCE OUTPUT 1</Para>
<Para>BALANCE INPUT</Para>
<Para>BALANCE INPUT</Para>
<Para>BALANCE OUTPUT 2</Para>
<Para>OP AMP INPUT</Para>
<Para>OP AMP OUTPUT</Para>
<Para>OP AMP INVERTED INPUT</Para>
<Para>TRACK CROSSSIGNAL</Para>
<Para>TRACKING ON</Para>
<Para>TRAVERSE SERVO ON</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<Table frame="ALL" colsep="1" rowsep="1"><tgroup cols="3" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.394in"><colspec colnum="2" colname="2" colwidth="0.787in"><colspec colnum="3" colname="3" colwidth="2.165in"><thead><row rowsep="1"><entry namest="1" nameend="2" align="CENTER"><Para>INITIAL&sol;LOGO</Para>
</entry>
<entry colname="3" align="CENTER"><Para>ABBREVIATIONS</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="CENTER"><Para>V</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>VBLANK</Para>
<Para>VCC</Para>
<Para></Para>
<Para>VCDCONT</Para>
<Para></Para>
<Para>VDD</Para>
<Para>VFB</Para>
<Para>VREF</Para>
<Para>VSS</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>V BLANKING</Para>
<Para>COLLECTOR POWER SUPPLY</Para>
<Para>VOLTAGE</Para>
<Para>VIDEO CD CONTROL (TRACKING</Para>
<Para>BALANCE)</Para>
<Para>DRAIN POWER SUPPLY VOLTAGE</Para>
<Para>VIDEO FEED BACK</Para>
<Para>VOLTAGE REFERENCE</Para>
<Para>SOURCE POWER SUPPLYVOLTAGE</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="CENTER"><Para>W</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>WAIT</Para>
<Para>WDCK</Para>
<Para>WEH</Para>
<Para>WSR</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>BUS CYCLE WAIT</Para>
<Para>WORD CLOCK</Para>
<Para>WRITE ENABLE HIGH</Para>
<Para>WORD SELECT RECEIVER</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="CENTER"><Para>X</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para>X</Para>
<Para>XALE</Para>
<Para>XAREQ</Para>
<Para>XCDROM</Para>
<Para>XCS</Para>
<Para>XCSYNC</Para>
<Para>XDS</Para>
<Para>XHSYNCO</Para>
<Para>XHINT</Para>
<Para>XI</Para>
<Para>XINT</Para>
<Para>XMW</Para>
<Para>XO</Para>
<Para>XRE</Para>
<Para>XSRMCE</Para>
<Para>XSRMOE</Para>
<Para>XSRMWE</Para>
<Para>XVCS</Para>
<Para>XVDS</Para>
<Para>XVSYNCO</Para>
</entry>
<entry colname="3" align="JUSTIFY"><Para>X&apos; TAL</Para>
<Para>X ADDRESS LATCH ENABLE</Para>
<Para>X AUDIO DATA REQUEST</Para>
<Para>X CD ROM CHIP SELECT</Para>
<Para>X CHIP SELECT</Para>
<Para>X COMPOSITE SYNC</Para>
<Para>X DATA STROBE</Para>
<Para>X HORIZONTAL SYNC OUTPUT</Para>
<Para>XH INTERRUPTREQUEST</Para>
<Para>X&apos; TAL OSCILLATOR INPUT</Para>
<Para>X INTERRUPT</Para>
<Para>X MEMORY WRITE ENABLE</Para>
<Para>X&apos; TAL OSCILLATOR OUTPUT</Para>
<Para>X READ ENABLE</Para>
<Para>X SRAM CHIP ENABLE</Para>
<Para>X SRAM OUTPUT ENABLE</Para>
<Para>X SRAM WRITE ENABLE</Para>
<Para>X V-DEC CHIPSELECT</Para>
<Para>X V-DEC CONTROL BUS STROBE</Para>
<Para>X VERTICAL SYNC OUTPUT</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<!-- Footer -->
<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
rv20u
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s1202000000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s1400000000x
</nmlist>
</nameloc>
</Para>
</Descriptive>
&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
