ContentsPreviousNext
Settings

# Printing on Inkjet Transparency

Follow the procedure below to print on inkjet transparency.

- Ink on an inkjet transparency takes some time to dry. We recommend that you remove a printed inkjet transparency from the output tray before the next inkjet transparency is delivered.

- The print delivery time interval can be set longer to avoid printed inkjet transparency from sticking together due to wet ink.

Lift the output tray.

When the output tray is lifted, the paper tray will pop out slightly.

Hold both sides of the paper tray, and pull it toward you.

- The paper tray cannot be detached. Do not pull it forcefully.

Squeeze the paper guide release, and then slide the side paper guides into position according to the inkjet transparency size.

- Beforehand, make sure to squeeze the front end paper guide, and then expand the guide.

Load inkjet transparency into the paper tray with the notched corner in the right front corner of the tray. Do not load transparencies over the limit mark.

- Curled inkjet transparency may jam. Straighten any curls before loading.

- If other paper is loaded, remove it, and then load inkjet transparency.

- To prevent the leading edge of transparencies from being scratched, place transparencies one at a time.

Squeeze the front end paper guide, and then slide it to meet the edge of the inkjet transparency.

Hold both sides of the paper tray, and push it gently in until it stops.

Lower the output tray.

Slide the envelope selector to the forward position .

Open the printer properties dialog box from the application.

On the [Setup] tab, click [Inkjet Transparency] in the [Paper type:] list.

Make the necessary settings, and then click [OK].

The printer properties dialog box closes.

Make print settings, and then click [OK].

- Opening from an Application

- Paper Handling Precautions