ContentsPreviousNext
Settings

# Printing on Semi-gloss Photo Paper

Follow the procedure below to print on semi-gloss photo paper.

Lift the output tray.

When the output tray is lifted, the paper tray will pop out slightly.

Hold both sides of the paper tray, and pull it toward you.

- The paper tray cannot be detached. Do not pull it forcefully.

Squeeze the paper guide release, and then slide the side paper guides into position according to the paper size.

- Beforehand, make sure to squeeze the front end paper guide, and then expand the guide.

Load semi-gloss photo paper with the print side face down but not over the limit mark.

- The print side is rough and white-coated.

- Curled paper may jam. Straighten any curls before loading.

Squeeze the front end paper guide, and then slide it to meet the edge of the paper.

Hold both sides of the paper tray, and push it gently in until it stops.

Lower the output tray.

Slide the envelope selector to the forward position .

Open the printer properties dialog box from the application.

On the [Setup] tab, click [Semi-gloss Photo Paper] in the [Paper type:] list.

Make the necessary settings, and then click [OK].

The printer properties dialog box closes.

Make print settings, and then click [OK].

- The output tray can hold up to 20 sheets of semi-gloss photo paper at a time.

- Opening from an Application

- Paper Handling Precautions